<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.1">
<drawing>
<board>
<plain>
<wire x1="72.5" y1="-6" x2="3" y2="-6" width="0.1524" layer="20"/>
<wire x1="0" y1="-3" x2="0" y2="103.5" width="0.1524" layer="20"/>
<wire x1="3" y1="106.5" x2="72.5" y2="106.5" width="0.1524" layer="20"/>
<wire x1="72.5" y1="106.5" x2="73.5" y2="105.5" width="0.1524" layer="20" curve="-90"/>
<wire x1="73.5" y1="105.5" x2="73.5" y2="-5" width="0.1524" layer="20"/>
<wire x1="73.5" y1="-5" x2="72.5" y2="-6" width="0.1524" layer="20" curve="-90"/>
<text>pwr</text>
<text>clk</text>
<text>err</text>
<text>reset</text>
<text>tx bridge</text>
<text>rx bridge</text>
<text>rx atk</text>
<text>tx atk</text>
<text>ATKP4</text>
<text>ATKP3</text>
<text>ATKP2</text>
<text>ATKP1</text>
<text>ATKP0</text>
<text>atkrouter v0.21
https://gitlab.cba.mit.edu/jakeread/automatakit</text>
<text>big open spaces
are like endless durations
until you find it</text>
<wire x1="0" y1="-3" x2="3" y2="-6" width="0.1524" layer="20" curve="90"/>
<wire x1="3" y1="106.5" x2="0" y2="103.5" width="0.1524" layer="20" curve="90"/>
<text>GND</text>
<text>ATKP5</text>
<text>VCC</text>
<text>cut for no usb power from host</text>
<text>&lt; pwr rpi | pwr brd &gt;</text>
<text>&lt; pwr to rpi</text>
<text>&lt; pwr from rpi</text>
<text>gnd &gt;</text>
<text>usbdp</text>
<text>usbdm</text>
</plain>
<libraries>
<library name="lights">
<packages>
<package name="LED0805">
</package>
</packages>
</library>
<library name="connector">
<packages>
<package name="JRTOMBSTONE">
</package>
<package name="DX4R005HJ5">
</package>
<package name="RASPBERRYPI-3BPLUS">
</package>
<package name="POGO">
</package>
<package name="CBA-SILK-LOGO">
</package>
<package name="FIDUCIAL_1MM">
</package>
<package name="SJFAB">
</package>
<package name="RJ45-LED-RJHSE-5381-UPTAB">
</package>
</packages>
</library>
<library name="microcontrollers">
<packages>
<package name="QFN-64-9X9MM">
<description>&lt;h3&gt;64-pin QFN 9x9mm, 0.5mm pitch&lt;/h3&gt;
&lt;p&gt;Package used by ATmega128RFA1&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.atmel.com/Images/Atmel-8266-MCU_Wireless-ATmega128RFA1_Datasheet.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
<package name="PDI_2X3_SMD">
<description>&lt;h3&gt;Surface Mount - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:2.54mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="QFN-24_ALT2">
<description>&lt;h3&gt;24-pin QFN with Exposed Thermal pad&lt;/h3&gt;
Parts that use this package:
&lt;ul&gt;
&lt;li&gt;A6282&lt;/li&gt;
&lt;/ul&gt;
Last modified: 8/20/10&lt;br&gt;
&lt;br&gt;
&lt;b&gt;***UNPROVEN***&lt;/b&gt;&lt;BR&gt;</description>
</package>
</packages>
</library>
<library name="power">
<packages>
<package name="PWRPAD_M25_STANDOFF">
</package>
<package name="NPTH-3-25MM">
</package>
<package name="PWRPAD_M3_STANDOFF">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
<package name="QFN16-3X3-TI-RTE">
<description>3x3 mm</description>
</package>
<package name="NRS5020T4R7MMGJ">
</package>
</packages>
</library>
<library name="passives">
<packages>
<package name="TACT-SWITCH-KMR6">
</package>
<package name="0805">
</package>
<package name="0603-CAP">
</package>
<package name="1206">
</package>
<package name="RES_PRQC">
</package>
<package name="SOD-123HE">
</package>
</packages>
</library>
<library name="comm">
<packages>
<package name="TSSOP16">
<description>&lt;b&gt;TSOP16&lt;/b&gt;&lt;p&gt;
thin small outline package</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="SLIDESWITCH-CL-SB-22A">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="D2" library="lights" package="LED0805" value="LED0805RX"/>
<element name="MP1" library="connector" package="JRTOMBSTONE" value="JRTOMBSTONE"/>
<element name="U3" library="microcontrollers" package="QFN-64-9X9MM" value="ATXMEGA_A3UQFN"/>
<element name="J10" library="power" package="PWRPAD_M25_STANDOFF" value="PWRPADM2.5_STANDOFF"/>
<element name="S1" library="passives" package="TACT-SWITCH-KMR6" value="2-8X4-5_SWITCH"/>
<element name="R6" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="C8" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="X1" library="connector" package="DX4R005HJ5" value="MICRO-USB_ORIG"/>
<element name="Y1" library="passives" package="RES_PRQC" value="RESONATORPQRC"/>
<element name="J5" library="microcontrollers" package="PDI_2X3_SMD" value="">
<attribute name="PROD_ID" value="CONN-11290"/>
</element>
<element name="R7" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R8" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="C5" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C4" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C3" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C2" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="U1" library="connector" package="RASPBERRYPI-3BPLUS" value="RASPBERRYPI-3BPLUS"/>
<element name="J11" library="power" package="PWRPAD_M25_STANDOFF" value="PWRPADM2.5_STANDOFF"/>
<element name="J2" library="connector" package="POGO" value="POGO"/>
<element name="J4" library="connector" package="POGO" value="POGO"/>
<element name="J6" library="connector" package="POGO" value="POGO"/>
<element name="J3" library="connector" package="POGO" value="POGO"/>
<element name="C10" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C7" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="D3" library="lights" package="LED0805" value="LED0805TX"/>
<element name="R2" library="passives" package="0805" value="1k">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R3" library="passives" package="0805" value="1k">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="D6" library="lights" package="LED0805" value="LED0805RX"/>
<element name="R5" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="D5" library="lights" package="LED0805" value="LED0805RX"/>
<element name="R4" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="D4" library="lights" package="LED0805" value="LED0805RX"/>
<element name="U$2" library="connector" package="CBA-SILK-LOGO" value="CBA-LOGO"/>
<element name="J1" library="connector" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="J22" library="connector" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U5" library="microcontrollers" package="QFN-24_ALT2" value="CP2102N"/>
<element name="R1" library="passives" package="0805" value="10k">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="M1" library="power" package="NPTH-3-25MM" value="M3-NPTH"/>
<element name="M2" library="power" package="NPTH-3-25MM" value="M3-NPTH"/>
<element name="M3" library="power" package="NPTH-3-25MM" value="M3-NPTH"/>
<element name="M4" library="power" package="NPTH-3-25MM" value="M3-NPTH"/>
<element name="J9" library="power" package="PWRPAD_M3_STANDOFF" value="PWRPADM3-STANDOFF"/>
<element name="U2" library="power" package="SOT23-5" value="VREG-AP2112"/>
<element name="C9" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C14" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C13" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="U6" library="comm" package="TSSOP16" value="RS485-2BY2-SN75C1168PWR"/>
<element name="R19" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R20" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="C22" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="R9" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R10" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="U7" library="comm" package="TSSOP16" value="RS485-2BY2-SN75C1168PWR"/>
<element name="R21" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R22" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="C23" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="R11" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R12" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="U8" library="comm" package="TSSOP16" value="RS485-2BY2-SN75C1168PWR"/>
<element name="R23" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R24" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="C24" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="R13" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R14" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="U9" library="comm" package="TSSOP16" value="RS485-2BY2-SN75C1168PWR"/>
<element name="R25" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R26" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="C25" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="R15" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R16" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="U10" library="comm" package="TSSOP16" value="RS485-2BY2-SN75C1168PWR"/>
<element name="R27" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R28" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="C26" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="R17" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R18" library="passives" package="0805" value="470R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="U11" library="comm" package="TSSOP16" value="RS485-2BY2-SN75C1168PWR"/>
<element name="R29" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R30" library="passives" package="0805" value="120R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="C27" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="J12" library="power" package="PWRPAD_M25_STANDOFF" value="PWRPADM2.5_STANDOFF"/>
<element name="J13" library="power" package="PWRPAD_M25_STANDOFF" value="PWRPADM2.5_STANDOFF"/>
<element name="J8" library="power" package="PWRPAD_M3_STANDOFF" value="PWRPADM3-STANDOFF"/>
<element name="J15" library="connector" package="POGO" value="POGO"/>
<element name="C6" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C11" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C1" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="U4" library="power" package="QFN16-3X3-TI-RTE" value="BUCK-TS30011-12-13QFN"/>
<element name="L1" library="power" package="NRS5020T4R7MMGJ" value="4.7uH"/>
<element name="S2" library="fab" package="SLIDESWITCH-CL-SB-22A" value="SLIDE-SWITCHSMT"/>
<element name="C15" library="passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C16" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C17" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C18" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C19" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C20" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C21" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C12" library="passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="D1" library="passives" package="SOD-123HE" value=""/>
<element name="J14" library="SparkFun-Connectors" package="1X04_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-09696"/>
</element>
<element name="J7" library="connector" package="SJFAB" value="SOLDER_JUMPER"/>
<element name="J16" library="connector" package="RJ45-LED-RJHSE-5381-UPTAB" value="ATK-RS48PHYVERJ45LEDTABUP"/>
<element name="J17" library="connector" package="RJ45-LED-RJHSE-5381-UPTAB" value="ATK-RS48PHYVERJ45LEDTABUP"/>
<element name="J18" library="connector" package="RJ45-LED-RJHSE-5381-UPTAB" value="ATK-RS48PHYVERJ45LEDTABUP"/>
<element name="J19" library="connector" package="RJ45-LED-RJHSE-5381-UPTAB" value="ATK-RS48PHYVERJ45LEDTABUP"/>
<element name="J20" library="connector" package="RJ45-LED-RJHSE-5381-UPTAB" value="ATK-RS48PHYVERJ45LEDTABUP"/>
<element name="J21" library="connector" package="RJ45-LED-RJHSE-5381-UPTAB" value="ATK-RS48PHYVERJ45LEDTABUP"/>
</elements>
<signals>
<signal name="ATK0-RXLED">
<contactref element="R7" pad="1"/>
<contactref element="U3" pad="46"/>
</signal>
<signal name="ATK0-TXLED">
<contactref element="R8" pad="1"/>
<contactref element="U3" pad="47"/>
</signal>
<signal name="ATK0-TX">
<contactref element="U6" pad="15"/>
<contactref element="U3" pad="49"/>
</signal>
<signal name="ATK0-RX">
<contactref element="U6" pad="5"/>
<contactref element="U3" pad="48"/>
</signal>
<signal name="+3V3">
<contactref element="U3" pad="15"/>
<contactref element="U3" pad="45"/>
<contactref element="U3" pad="35"/>
<contactref element="U3" pad="25"/>
<contactref element="U3" pad="53"/>
<contactref element="C8" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="U3" pad="61"/>
<contactref element="J5" pad="2"/>
<contactref element="C10" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="D6" pad="1"/>
<contactref element="D5" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="U5" pad="5"/>
<contactref element="U5" pad="7"/>
<contactref element="U5" pad="6"/>
<contactref element="R1" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="C14" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="U6" pad="4"/>
<contactref element="U6" pad="12"/>
<contactref element="U7" pad="4"/>
<contactref element="U7" pad="12"/>
<contactref element="U8" pad="4"/>
<contactref element="U8" pad="12"/>
<contactref element="U9" pad="4"/>
<contactref element="U9" pad="12"/>
<contactref element="U10" pad="4"/>
<contactref element="U10" pad="12"/>
<contactref element="U11" pad="4"/>
<contactref element="U11" pad="12"/>
<contactref element="C1" pad="1"/>
<contactref element="J16" pad="GRNP"/>
<contactref element="J16" pad="YLWP"/>
<contactref element="J17" pad="GRNP"/>
<contactref element="J17" pad="YLWP"/>
<contactref element="J18" pad="GRNP"/>
<contactref element="J18" pad="YLWP"/>
<contactref element="J19" pad="GRNP"/>
<contactref element="J19" pad="YLWP"/>
<contactref element="J20" pad="GRNP"/>
<contactref element="J20" pad="YLWP"/>
<contactref element="J21" pad="GRNP"/>
<contactref element="J21" pad="YLWP"/>
</signal>
<signal name="GND">
<contactref element="U3" pad="60"/>
<contactref element="U3" pad="52"/>
<contactref element="U3" pad="44"/>
<contactref element="U3" pad="P$1"/>
<contactref element="U3" pad="34"/>
<contactref element="U3" pad="24"/>
<contactref element="U3" pad="14"/>
<contactref element="C8" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="Y1" pad="2"/>
<contactref element="J5" pad="6"/>
<contactref element="S1" pad="P$2"/>
<contactref element="X1" pad="GND"/>
<contactref element="J3" pad="P$1"/>
<contactref element="C10" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R6" pad="1"/>
<contactref element="U5" pad="2"/>
<contactref element="U5" pad="EP"/>
<contactref element="U2" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="U6" pad="8"/>
<contactref element="C22" pad="2"/>
<contactref element="U7" pad="8"/>
<contactref element="C23" pad="2"/>
<contactref element="U8" pad="8"/>
<contactref element="C24" pad="2"/>
<contactref element="U9" pad="8"/>
<contactref element="C25" pad="2"/>
<contactref element="U10" pad="8"/>
<contactref element="C26" pad="2"/>
<contactref element="U11" pad="8"/>
<contactref element="C27" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="U4" pad="4"/>
<contactref element="U4" pad="TH"/>
<contactref element="U4" pad="15"/>
<contactref element="U4" pad="14"/>
<contactref element="J9" pad="P$1"/>
<contactref element="C16" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C19" pad="2"/>
<contactref element="C20" pad="2"/>
<contactref element="C21" pad="1"/>
<contactref element="C12" pad="2"/>
<contactref element="D1" pad="P$2"/>
<contactref element="J14" pad="1"/>
</signal>
<signal name="ATK1-RX">
<contactref element="U7" pad="5"/>
<contactref element="U3" pad="42"/>
</signal>
<signal name="ATK1-TX">
<contactref element="U7" pad="15"/>
<contactref element="U3" pad="43"/>
</signal>
<signal name="ATK1-RXLED">
<contactref element="R9" pad="1"/>
<contactref element="U3" pad="40"/>
</signal>
<signal name="ATK1-TXLED">
<contactref element="R10" pad="1"/>
<contactref element="U3" pad="41"/>
</signal>
<signal name="ATK2-RX">
<contactref element="U8" pad="5"/>
<contactref element="U3" pad="38"/>
</signal>
<signal name="ATK2-TX">
<contactref element="U8" pad="15"/>
<contactref element="U3" pad="39"/>
</signal>
<signal name="ATK2-RXLED">
<contactref element="R11" pad="1"/>
<contactref element="U3" pad="36"/>
</signal>
<signal name="ATK2-TXLED">
<contactref element="R12" pad="1"/>
<contactref element="U3" pad="37"/>
</signal>
<signal name="ATK3-RX">
<contactref element="U9" pad="5"/>
<contactref element="U3" pad="32"/>
</signal>
<signal name="ATK3-TX">
<contactref element="U9" pad="15"/>
<contactref element="U3" pad="33"/>
</signal>
<signal name="ATK3-RXLED">
<contactref element="R13" pad="1"/>
<contactref element="U3" pad="30"/>
</signal>
<signal name="ATK3-TXLED">
<contactref element="R14" pad="1"/>
<contactref element="U3" pad="31"/>
</signal>
<signal name="ATK4-RX">
<contactref element="U10" pad="5"/>
<contactref element="U3" pad="28"/>
</signal>
<signal name="ATK4-TX">
<contactref element="U10" pad="15"/>
<contactref element="U3" pad="29"/>
</signal>
<signal name="ATK4-RXLED">
<contactref element="R15" pad="1"/>
<contactref element="U3" pad="26"/>
</signal>
<signal name="ATK4-TXLED">
<contactref element="R16" pad="1"/>
<contactref element="U3" pad="27"/>
</signal>
<signal name="ATK0-CLKIN">
<contactref element="U6" pad="3"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="PDI_DATA">
<contactref element="U3" pad="56"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="RESET/PDI_CLK">
<contactref element="U3" pad="57"/>
<contactref element="J5" pad="5"/>
<contactref element="S1" pad="P$4"/>
</signal>
<signal name="N$13">
<contactref element="Y1" pad="1"/>
<contactref element="U3" pad="58"/>
</signal>
<signal name="N$14">
<contactref element="U3" pad="59"/>
<contactref element="Y1" pad="3"/>
</signal>
<signal name="DM">
<contactref element="X1" pad="D-"/>
<contactref element="J6" pad="P$1"/>
<contactref element="U5" pad="4"/>
</signal>
<signal name="DP">
<contactref element="X1" pad="D+"/>
<contactref element="J4" pad="P$1"/>
<contactref element="U5" pad="3"/>
</signal>
<signal name="CPRX">
<contactref element="U3" pad="18"/>
<contactref element="U5" pad="21"/>
</signal>
<signal name="CPTX">
<contactref element="U3" pad="19"/>
<contactref element="U5" pad="20"/>
</signal>
<signal name="N$19">
<contactref element="U5" pad="9"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="CPTXLED">
<contactref element="R3" pad="1"/>
<contactref element="U5" pad="14"/>
</signal>
<signal name="CPRXLED">
<contactref element="R2" pad="1"/>
<contactref element="U5" pad="13"/>
</signal>
<signal name="N$37">
<contactref element="R2" pad="2"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="R3" pad="2"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="D6" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="D5" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="STLCLK">
<contactref element="R5" pad="1"/>
<contactref element="U3" pad="62"/>
</signal>
<signal name="N$21">
<contactref element="D4" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="STLERR">
<contactref element="R4" pad="1"/>
<contactref element="U3" pad="63"/>
</signal>
<signal name="ATK-CLKOUT">
<contactref element="U6" pad="9"/>
<contactref element="U7" pad="9"/>
<contactref element="U8" pad="9"/>
<contactref element="U9" pad="9"/>
<contactref element="U10" pad="9"/>
<contactref element="U11" pad="9"/>
<contactref element="U3" pad="50"/>
</signal>
<signal name="TX-Y">
<contactref element="U6" pad="14"/>
<contactref element="J16" pad="P$6"/>
</signal>
<signal name="TX-Z">
<contactref element="U6" pad="13"/>
<contactref element="J16" pad="P$5"/>
</signal>
<signal name="RX-B">
<contactref element="U6" pad="7"/>
<contactref element="R20" pad="1"/>
<contactref element="J16" pad="P$4"/>
</signal>
<signal name="RX-A">
<contactref element="R20" pad="2"/>
<contactref element="U6" pad="6"/>
<contactref element="J16" pad="P$3"/>
</signal>
<signal name="CLKRX-A">
<contactref element="U6" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="J16" pad="P$8"/>
</signal>
<signal name="CLKRX-B">
<contactref element="R19" pad="2"/>
<contactref element="U6" pad="1"/>
<contactref element="J16" pad="P$7"/>
</signal>
<signal name="CLKTX-Z">
<contactref element="U6" pad="11"/>
<contactref element="J16" pad="P$2"/>
</signal>
<signal name="CLKRX-Y">
<contactref element="U6" pad="10"/>
<contactref element="J16" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="R7" pad="2"/>
<contactref element="J16" pad="GRNN"/>
</signal>
<signal name="N$2">
<contactref element="R8" pad="2"/>
<contactref element="J16" pad="YLWN"/>
</signal>
<signal name="+5V">
<contactref element="U5" pad="8"/>
<contactref element="C9" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="3"/>
<contactref element="C22" pad="1"/>
<contactref element="U6" pad="16"/>
<contactref element="C23" pad="1"/>
<contactref element="U7" pad="16"/>
<contactref element="C24" pad="1"/>
<contactref element="U8" pad="16"/>
<contactref element="C25" pad="1"/>
<contactref element="U9" pad="16"/>
<contactref element="C26" pad="1"/>
<contactref element="U10" pad="16"/>
<contactref element="C27" pad="1"/>
<contactref element="U11" pad="16"/>
<contactref element="C6" pad="1"/>
<contactref element="C11" pad="2"/>
<contactref element="S2" pad="P$6"/>
<contactref element="S2" pad="P$3"/>
<contactref element="X1" pad="VBUS"/>
<contactref element="J7" pad="1"/>
<contactref element="J7" pad="2"/>
<contactref element="J2" pad="P$1"/>
</signal>
<signal name="N$25">
<contactref element="U7" pad="14"/>
<contactref element="J17" pad="P$6"/>
</signal>
<signal name="N$26">
<contactref element="U7" pad="13"/>
<contactref element="J17" pad="P$5"/>
</signal>
<signal name="N$27">
<contactref element="U7" pad="7"/>
<contactref element="R22" pad="1"/>
<contactref element="J17" pad="P$4"/>
</signal>
<signal name="N$28">
<contactref element="R22" pad="2"/>
<contactref element="U7" pad="6"/>
<contactref element="J17" pad="P$3"/>
</signal>
<signal name="N$29">
<contactref element="U7" pad="2"/>
<contactref element="R21" pad="1"/>
<contactref element="J17" pad="P$8"/>
</signal>
<signal name="N$30">
<contactref element="R21" pad="2"/>
<contactref element="U7" pad="1"/>
<contactref element="J17" pad="P$7"/>
</signal>
<signal name="N$31">
<contactref element="U7" pad="11"/>
<contactref element="J17" pad="P$2"/>
</signal>
<signal name="N$32">
<contactref element="U7" pad="10"/>
<contactref element="J17" pad="P$1"/>
</signal>
<signal name="N$33">
<contactref element="R9" pad="2"/>
<contactref element="J17" pad="GRNN"/>
</signal>
<signal name="N$34">
<contactref element="R10" pad="2"/>
<contactref element="J17" pad="YLWN"/>
</signal>
<signal name="N$3">
<contactref element="U8" pad="14"/>
<contactref element="J18" pad="P$6"/>
</signal>
<signal name="N$4">
<contactref element="U8" pad="13"/>
<contactref element="J18" pad="P$5"/>
</signal>
<signal name="N$5">
<contactref element="U8" pad="7"/>
<contactref element="R24" pad="1"/>
<contactref element="J18" pad="P$4"/>
</signal>
<signal name="N$6">
<contactref element="R24" pad="2"/>
<contactref element="U8" pad="6"/>
<contactref element="J18" pad="P$3"/>
</signal>
<signal name="N$7">
<contactref element="U8" pad="2"/>
<contactref element="R23" pad="1"/>
<contactref element="J18" pad="P$8"/>
</signal>
<signal name="N$8">
<contactref element="R23" pad="2"/>
<contactref element="U8" pad="1"/>
<contactref element="J18" pad="P$7"/>
</signal>
<signal name="N$9">
<contactref element="U8" pad="11"/>
<contactref element="J18" pad="P$2"/>
</signal>
<signal name="N$10">
<contactref element="U8" pad="10"/>
<contactref element="J18" pad="P$1"/>
</signal>
<signal name="N$35">
<contactref element="R11" pad="2"/>
<contactref element="J18" pad="GRNN"/>
</signal>
<signal name="N$36">
<contactref element="R12" pad="2"/>
<contactref element="J18" pad="YLWN"/>
</signal>
<signal name="N$39">
<contactref element="U9" pad="14"/>
<contactref element="J19" pad="P$6"/>
</signal>
<signal name="N$40">
<contactref element="U9" pad="13"/>
<contactref element="J19" pad="P$5"/>
</signal>
<signal name="N$41">
<contactref element="U9" pad="7"/>
<contactref element="R26" pad="1"/>
<contactref element="J19" pad="P$4"/>
</signal>
<signal name="N$42">
<contactref element="R26" pad="2"/>
<contactref element="U9" pad="6"/>
<contactref element="J19" pad="P$3"/>
</signal>
<signal name="N$43">
<contactref element="U9" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="J19" pad="P$8"/>
</signal>
<signal name="N$44">
<contactref element="R25" pad="2"/>
<contactref element="U9" pad="1"/>
<contactref element="J19" pad="P$7"/>
</signal>
<signal name="N$45">
<contactref element="U9" pad="11"/>
<contactref element="J19" pad="P$2"/>
</signal>
<signal name="N$46">
<contactref element="U9" pad="10"/>
<contactref element="J19" pad="P$1"/>
</signal>
<signal name="N$47">
<contactref element="R13" pad="2"/>
<contactref element="J19" pad="GRNN"/>
</signal>
<signal name="N$48">
<contactref element="R14" pad="2"/>
<contactref element="J19" pad="YLWN"/>
</signal>
<signal name="N$49">
<contactref element="U10" pad="14"/>
<contactref element="J20" pad="P$6"/>
</signal>
<signal name="N$50">
<contactref element="U10" pad="13"/>
<contactref element="J20" pad="P$5"/>
</signal>
<signal name="N$51">
<contactref element="U10" pad="7"/>
<contactref element="R28" pad="1"/>
<contactref element="J20" pad="P$4"/>
</signal>
<signal name="N$52">
<contactref element="R28" pad="2"/>
<contactref element="U10" pad="6"/>
<contactref element="J20" pad="P$3"/>
</signal>
<signal name="N$53">
<contactref element="U10" pad="2"/>
<contactref element="R27" pad="1"/>
<contactref element="J20" pad="P$8"/>
</signal>
<signal name="N$54">
<contactref element="R27" pad="2"/>
<contactref element="U10" pad="1"/>
<contactref element="J20" pad="P$7"/>
</signal>
<signal name="N$55">
<contactref element="U10" pad="11"/>
<contactref element="J20" pad="P$2"/>
</signal>
<signal name="N$56">
<contactref element="U10" pad="10"/>
<contactref element="J20" pad="P$1"/>
</signal>
<signal name="N$57">
<contactref element="R15" pad="2"/>
<contactref element="J20" pad="GRNN"/>
</signal>
<signal name="N$58">
<contactref element="R16" pad="2"/>
<contactref element="J20" pad="YLWN"/>
</signal>
<signal name="N$59">
<contactref element="U11" pad="14"/>
<contactref element="J21" pad="P$6"/>
</signal>
<signal name="N$60">
<contactref element="U11" pad="13"/>
<contactref element="J21" pad="P$5"/>
</signal>
<signal name="N$61">
<contactref element="U11" pad="7"/>
<contactref element="R30" pad="1"/>
<contactref element="J21" pad="P$4"/>
</signal>
<signal name="N$62">
<contactref element="R30" pad="2"/>
<contactref element="U11" pad="6"/>
<contactref element="J21" pad="P$3"/>
</signal>
<signal name="N$63">
<contactref element="U11" pad="2"/>
<contactref element="R29" pad="1"/>
<contactref element="J21" pad="P$8"/>
</signal>
<signal name="N$64">
<contactref element="R29" pad="2"/>
<contactref element="U11" pad="1"/>
<contactref element="J21" pad="P$7"/>
</signal>
<signal name="N$65">
<contactref element="U11" pad="11"/>
<contactref element="J21" pad="P$2"/>
</signal>
<signal name="N$66">
<contactref element="U11" pad="10"/>
<contactref element="J21" pad="P$1"/>
</signal>
<signal name="N$67">
<contactref element="R17" pad="2"/>
<contactref element="J21" pad="GRNN"/>
</signal>
<signal name="N$68">
<contactref element="R18" pad="2"/>
<contactref element="J21" pad="YLWN"/>
</signal>
<signal name="ATK1-CLKIN">
<contactref element="U7" pad="3"/>
<contactref element="U3" pad="2"/>
</signal>
<signal name="ATK2-CLKIN">
<contactref element="U8" pad="3"/>
<contactref element="U3" pad="3"/>
</signal>
<signal name="ATK3-CLKIN">
<contactref element="U9" pad="3"/>
<contactref element="U3" pad="4"/>
</signal>
<signal name="ATK4-CLKIN">
<contactref element="U10" pad="3"/>
<contactref element="U3" pad="5"/>
</signal>
<signal name="ATK5-CLKIN">
<contactref element="U11" pad="3"/>
<contactref element="U3" pad="7"/>
</signal>
<signal name="ATK5-TX">
<contactref element="U11" pad="15"/>
<contactref element="U3" pad="23"/>
</signal>
<signal name="ATK5-RX">
<contactref element="U11" pad="5"/>
<contactref element="U3" pad="22"/>
</signal>
<signal name="ATK5-RXLED">
<contactref element="R17" pad="1"/>
<contactref element="U3" pad="20"/>
</signal>
<signal name="ATK5-TXLED">
<contactref element="R18" pad="1"/>
<contactref element="U3" pad="21"/>
</signal>
<signal name="5VBUCK">
<contactref element="U4" pad="5"/>
<contactref element="L1" pad="1"/>
<contactref element="C16" pad="1"/>
<contactref element="C17" pad="1"/>
<contactref element="C18" pad="1"/>
<contactref element="C19" pad="1"/>
<contactref element="C20" pad="1"/>
<contactref element="S2" pad="P$5"/>
<contactref element="S2" pad="P$2"/>
</signal>
<signal name="VSW">
<contactref element="U4" pad="12"/>
<contactref element="U4" pad="1"/>
<contactref element="U4" pad="16"/>
<contactref element="U4" pad="13"/>
<contactref element="L1" pad="2"/>
<contactref element="C15" pad="1"/>
<contactref element="D1" pad="P$1"/>
</signal>
<signal name="VCC">
<contactref element="U4" pad="3"/>
<contactref element="U4" pad="2"/>
<contactref element="U4" pad="11"/>
<contactref element="J8" pad="P$1"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="BUCKBST">
<contactref element="U4" pad="10"/>
<contactref element="C15" pad="2"/>
</signal>
<signal name="N$69">
<contactref element="J15" pad="P$1"/>
<contactref element="C21" pad="2"/>
<contactref element="S2" pad="P$1"/>
<contactref element="S2" pad="P$4"/>
</signal>
<signal name="DBP3">
<contactref element="U3" pad="17"/>
<contactref element="J14" pad="4"/>
</signal>
<signal name="DBP2">
<contactref element="U3" pad="16"/>
<contactref element="J14" pad="3"/>
</signal>
<signal name="DBP1">
<contactref element="U3" pad="13"/>
<contactref element="J14" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
