<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.0">
<drawing>
<board>
<plain>
<text>UP1</text>
<text>UP2</text>
<text>UP3</text>
<text>UP4</text>
<text>UP0</text>
<text>mkrouter v0.6</text>
<text>ticker</text>
<text>pwr</text>
<text>packet</text>
<text>error</text>
<text>traceswo</text>
<text>swclk</text>
<text>swdio</text>
<text>reset</text>
<text>big empty spaces
feel like endless durations
until you find it </text>
<text>UP4</text>
<text>UP5</text>
<text>usb</text>
<wire x1="0" y1="88.6" x2="0" y2="3.6" width="0.2032" layer="20"/>
<wire x1="0" y1="3.6" x2="3.6" y2="0" width="0.2032" layer="20" curve="90"/>
<wire x1="3.6" y1="0" x2="75.8" y2="0" width="0.2032" layer="20"/>
<wire x1="75.8" y1="0" x2="76.6" y2="0.8" width="0.2032" layer="20" curve="90"/>
<wire x1="76.6" y1="0.8" x2="76.6" y2="4.2" width="0.2032" layer="20"/>
<wire x1="76.6" y1="4.2" x2="70" y2="5.4" width="0.2032" layer="20"/>
<wire x1="70" y1="5.4" x2="70" y2="9.6" width="0.2032" layer="20"/>
<wire x1="70" y1="9.6" x2="76.6" y2="10.8" width="0.2032" layer="20"/>
<wire x1="76.6" y1="10.8" x2="76.6" y2="19.2" width="0.2032" layer="20"/>
<wire x1="76.6" y1="19.2" x2="70" y2="20.4" width="0.2032" layer="20"/>
<wire x1="70" y1="20.4" x2="70" y2="24.6" width="0.2032" layer="20"/>
<wire x1="70" y1="24.6" x2="76.6" y2="25.8" width="0.2032" layer="20"/>
<wire x1="76.6" y1="25.8" x2="76.6" y2="34.2" width="0.2032" layer="20"/>
<wire x1="76.6" y1="34.2" x2="70" y2="35.4" width="0.2032" layer="20"/>
<wire x1="70" y1="35.4" x2="70" y2="39.6" width="0.2032" layer="20"/>
<wire x1="70" y1="39.6" x2="76.6" y2="40.8" width="0.2032" layer="20"/>
<wire x1="76.6" y1="40.8" x2="76.6" y2="49.2" width="0.2032" layer="20"/>
<wire x1="76.6" y1="49.2" x2="70" y2="50.4" width="0.2032" layer="20"/>
<wire x1="70" y1="50.4" x2="70" y2="54.6" width="0.2032" layer="20"/>
<wire x1="70" y1="54.6" x2="76.6" y2="55.8" width="0.2032" layer="20"/>
<wire x1="76.6" y1="55.8" x2="76.6" y2="64.2" width="0.2032" layer="20"/>
<wire x1="76.6" y1="64.2" x2="70" y2="65.4" width="0.2032" layer="20"/>
<wire x1="70" y1="65.4" x2="70" y2="69.6" width="0.2032" layer="20"/>
<wire x1="70" y1="69.6" x2="76.6" y2="70.8" width="0.2032" layer="20"/>
<wire x1="76.6" y1="70.8" x2="76.6" y2="79.2" width="0.2032" layer="20"/>
<wire x1="76.6" y1="79.2" x2="70" y2="80.4" width="0.2032" layer="20"/>
<wire x1="70" y1="80.4" x2="70" y2="84.6" width="0.2032" layer="20"/>
<wire x1="70" y1="84.6" x2="76.6" y2="85.8" width="0.2032" layer="20"/>
<wire x1="76.6" y1="85.8" x2="76.6" y2="91.4" width="0.2032" layer="20"/>
<wire x1="76.6" y1="91.4" x2="76" y2="92" width="0.2032" layer="20" curve="90"/>
<wire x1="76" y1="92" x2="38" y2="92" width="0.2032" layer="20"/>
<wire x1="17.9" y1="92" x2="3.4" y2="92" width="0.2032" layer="20"/>
<wire x1="3.4" y1="92" x2="0" y2="88.6" width="0.2032" layer="20" curve="90"/>
<wire x1="18" y1="92" x2="19" y2="91" width="0.2032" layer="20" curve="-90"/>
<wire x1="19" y1="91" x2="19" y2="85.5" width="0.2032" layer="20"/>
<wire x1="19" y1="85.5" x2="19.5" y2="85" width="0.2032" layer="20" curve="90"/>
<wire x1="19.5" y1="85" x2="36.5" y2="85" width="0.2032" layer="20"/>
<wire x1="36.5" y1="85" x2="37" y2="85.5" width="0.2032" layer="20" curve="90"/>
<wire x1="37" y1="85.5" x2="37" y2="91" width="0.2032" layer="20"/>
<wire x1="37" y1="91" x2="38" y2="92" width="0.2032" layer="20" curve="-90"/>
<text>UP0</text>
<text>UP1</text>
<text>UP2</text>
<text>UP3</text>
<text>UP4</text>
<text>UP5</text>
<text>usb power &lt; - &gt; external network power</text>
</plain>
<libraries>
<library name="fab">
<packages>
<package name="TACT-SWITCH-KMR6">
</package>
<package name="DX4R005HJ5">
</package>
<package name="CBA-SILK-LOGO">
</package>
<package name="MK-LOGO-SILK">
</package>
<package name="SLIDESWITCH-CL-SB-22A">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SAMTECH_FTSH-105-01">
<description>&lt;h3&gt;ARM Cortex Debug Connector (10-pin)&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.05"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.samtec.com/ftppub/cpdf/FTSH-1XX-XX-XXX-DV-XXX-MKT.pdf"&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CORTEX_DEBUG&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="borkedlabs-passives">
<packages>
<package name="1206">
</package>
<package name="0603-CAP">
</package>
<package name="0805">
</package>
</packages>
</library>
<library name="lights">
<packages>
<package name="LED0805">
</package>
</packages>
</library>
<library name="connector">
<packages>
<package name="RJ12-6-SMT">
</package>
<package name="RASPBERRYPI-3BPLUS">
</package>
<package name="POGO">
</package>
<package name="JRTOMBSTONE">
</package>
</packages>
</library>
<library name="microcontrollers">
<packages>
<package name="QFN-64-9X9MM">
<description>&lt;h3&gt;64-pin QFN 9x9mm, 0.5mm pitch&lt;/h3&gt;
&lt;p&gt;Package used by ATmega128RFA1&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.atmel.com/Images/Atmel-8266-MCU_Wireless-ATmega128RFA1_Datasheet.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="power">
<packages>
<package name="NRS5020T4R7MMGJ">
</package>
<package name="QFN16-3X3-TI-RTE">
<description>3x3 mm</description>
</package>
</packages>
</library>
<library name="borkedlabs-misc">
<packages>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="fab" package="TACT-SWITCH-KMR6" value="2-8X4-5_SWITCH"/>
<element name="X1" library="fab" package="DX4R005HJ5" value="MICRO-USB_ORIG"/>
<element name="C17" library="borkedlabs-passives" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C19" library="borkedlabs-passives" package="0603-CAP" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VALUE"/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="U$1" library="fab" package="CBA-SILK-LOGO" value=""/>
<element name="U$2" library="fab" package="MK-LOGO-SILK" value=""/>
<element name="R1" library="borkedlabs-passives" package="0805" value="10k">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="D13" library="lights" package="LED0805" value="LED0805"/>
<element name="D14" library="lights" package="LED0805" value="LED0805"/>
<element name="R14" library="borkedlabs-passives" package="0805" value="100R">
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="borkedlabs-passives" package="0805" value="150R">
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="lights" package="LED0805" value="LED0805"/>
<element name="D2" library="lights" package="LED0805" value="LED0805"/>
<element name="R2" library="borkedlabs-passives" package="0805" value="150R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R3" library="borkedlabs-passives" package="0805" value="100R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="J7" library="connector" package="RJ12-6-SMT" value="RJ12-6-SMT"/>
<element name="D3" library="lights" package="LED0805" value="LED0805"/>
<element name="D4" library="lights" package="LED0805" value="LED0805"/>
<element name="R4" library="borkedlabs-passives" package="0805" value="150R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R5" library="borkedlabs-passives" package="0805" value="100R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="J8" library="connector" package="RJ12-6-SMT" value="RJ12-6-SMT"/>
<element name="D5" library="lights" package="LED0805" value="LED0805"/>
<element name="D6" library="lights" package="LED0805" value="LED0805"/>
<element name="R6" library="borkedlabs-passives" package="0805" value="150R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R7" library="borkedlabs-passives" package="0805" value="100R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="J9" library="connector" package="RJ12-6-SMT" value="RJ12-6-SMT"/>
<element name="D7" library="lights" package="LED0805" value="LED0805"/>
<element name="D8" library="lights" package="LED0805" value="LED0805"/>
<element name="R8" library="borkedlabs-passives" package="0805" value="150R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R9" library="borkedlabs-passives" package="0805" value="100R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="J10" library="connector" package="RJ12-6-SMT" value="RJ12-6-SMT"/>
<element name="D9" library="lights" package="LED0805" value="LED0805"/>
<element name="D10" library="lights" package="LED0805" value="LED0805"/>
<element name="R10" library="borkedlabs-passives" package="0805" value="150R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R11" library="borkedlabs-passives" package="0805" value="100R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="J11" library="connector" package="RJ12-6-SMT" value="RJ12-6-SMT"/>
<element name="D12" library="lights" package="LED0805" value="LED0805"/>
<element name="R13" library="borkedlabs-passives" package="0805" value="150R">
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="lights" package="LED0805" value="LED0805"/>
<element name="R12" library="borkedlabs-passives" package="0805" value="150R">
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="SAMTECH_FTSH-105-01" value="CORTEX_DEBUG_SMD"/>
<element name="U1" library="microcontrollers" package="QFN-64-9X9MM" value="ATSAMD51QFN64"/>
<element name="C1" library="borkedlabs-passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C2" library="borkedlabs-passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C3" library="borkedlabs-passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C4" library="borkedlabs-passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C5" library="borkedlabs-passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C6" library="borkedlabs-passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C7" library="borkedlabs-passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="D15" library="lights" package="LED0805" value="LED0805"/>
<element name="D16" library="lights" package="LED0805" value="LED0805"/>
<element name="R16" library="borkedlabs-passives" package="0805" value="150R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="R17" library="borkedlabs-passives" package="0805" value="100R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
<element name="J1" library="connector" package="RJ12-6-SMT" value="RJ12-6-SMT"/>
<element name="C8" library="borkedlabs-passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C9" library="borkedlabs-passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="U3" library="connector" package="RASPBERRYPI-3BPLUS" value="RASPBERRYPI-3BPLUS"/>
<element name="J3" library="connector" package="POGO" value="POGO"/>
<element name="J4" library="connector" package="POGO" value="POGO"/>
<element name="J5" library="connector" package="POGO" value="POGO"/>
<element name="J6" library="connector" package="POGO" value="POGO"/>
<element name="L1" library="power" package="NRS5020T4R7MMGJ" value="4.7uF"/>
<element name="U$3" library="borkedlabs-misc" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U$4" library="borkedlabs-misc" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="U2" library="power" package="QFN16-3X3-TI-RTE" value="BUCK-TS30011-12-13QFN"/>
<element name="S3" library="fab" package="SLIDESWITCH-CL-SB-22A" value="SLIDE-SWITCHSMT"/>
<element name="C10" library="borkedlabs-passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C11" library="borkedlabs-passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C12" library="borkedlabs-passives" package="1206" value="10uF">
<attribute name="PACKAGE" value="1206"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="C13" library="borkedlabs-passives" package="0603-CAP" value="0.1uF">
<attribute name="PACKAGE" value="0603"/>
<attribute name="TYPE" value=""/>
<attribute name="VOLTAGE" value=""/>
</element>
<element name="MP1" library="connector" package="JRTOMBSTONE" value="JRTOMBSTONE"/>
<element name="D17" library="lights" package="LED0805" value="LED0805"/>
<element name="R18" library="borkedlabs-passives" package="0805" value="150R">
<attribute name="PACKAGE" value="0805"/>
<attribute name="PRECISION" value=""/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="X1" pad="GND"/>
<contactref element="J7" pad="P$4"/>
<contactref element="J7" pad="P$3"/>
<contactref element="J8" pad="P$4"/>
<contactref element="J8" pad="P$3"/>
<contactref element="J9" pad="P$4"/>
<contactref element="J9" pad="P$3"/>
<contactref element="J10" pad="P$4"/>
<contactref element="J10" pad="P$3"/>
<contactref element="J11" pad="P$4"/>
<contactref element="J11" pad="P$3"/>
<contactref element="R12" pad="1"/>
<contactref element="J2" pad="3"/>
<contactref element="J2" pad="5"/>
<contactref element="J2" pad="9"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="J1" pad="P$4"/>
<contactref element="J1" pad="P$3"/>
<contactref element="U1" pad="7"/>
<contactref element="U1" pad="22"/>
<contactref element="U1" pad="33"/>
<contactref element="U1" pad="47"/>
<contactref element="U1" pad="54"/>
<contactref element="J5" pad="P$1"/>
<contactref element="C17" pad="1"/>
<contactref element="S3" pad="P$6"/>
<contactref element="S3" pad="P$3"/>
<contactref element="U2" pad="14"/>
<contactref element="U2" pad="15"/>
<contactref element="U2" pad="TH"/>
<contactref element="U2" pad="4"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="S1" pad="P$3"/>
</signal>
<signal name="+3V3">
<contactref element="R1" pad="2"/>
<contactref element="D1" pad="1"/>
<contactref element="D2" pad="1"/>
<contactref element="J7" pad="P$6"/>
<contactref element="J7" pad="P$1"/>
<contactref element="D3" pad="1"/>
<contactref element="D4" pad="1"/>
<contactref element="J8" pad="P$6"/>
<contactref element="J8" pad="P$1"/>
<contactref element="D5" pad="1"/>
<contactref element="D6" pad="1"/>
<contactref element="J9" pad="P$6"/>
<contactref element="J9" pad="P$1"/>
<contactref element="D7" pad="1"/>
<contactref element="D8" pad="1"/>
<contactref element="J10" pad="P$6"/>
<contactref element="J10" pad="P$1"/>
<contactref element="D9" pad="1"/>
<contactref element="D10" pad="1"/>
<contactref element="J11" pad="P$6"/>
<contactref element="J11" pad="P$1"/>
<contactref element="D14" pad="1"/>
<contactref element="D13" pad="1"/>
<contactref element="D12" pad="1"/>
<contactref element="D11" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="D15" pad="1"/>
<contactref element="D16" pad="1"/>
<contactref element="J1" pad="P$6"/>
<contactref element="J1" pad="P$1"/>
<contactref element="U1" pad="8"/>
<contactref element="U1" pad="56"/>
<contactref element="U1" pad="48"/>
<contactref element="U1" pad="34"/>
<contactref element="U1" pad="21"/>
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="L1" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="U2" pad="5"/>
<contactref element="C13" pad="1"/>
<contactref element="D17" pad="1"/>
</signal>
<signal name="TRACESWO">
<contactref element="J2" pad="6"/>
<contactref element="U1" pad="59"/>
</signal>
<signal name="SWCLK">
<contactref element="J2" pad="4"/>
<contactref element="U1" pad="57"/>
</signal>
<signal name="SWDIO">
<contactref element="J2" pad="2"/>
<contactref element="U1" pad="58"/>
</signal>
<signal name="RESET">
<contactref element="R1" pad="1"/>
<contactref element="J2" pad="10"/>
<contactref element="U1" pad="52"/>
<contactref element="S1" pad="P$2"/>
</signal>
<signal name="UP1RX">
<contactref element="J8" pad="P$2"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="UP1TX">
<contactref element="J8" pad="P$5"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="UP1STLR">
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="42"/>
</signal>
<signal name="UP1STLB">
<contactref element="R5" pad="1"/>
<contactref element="U1" pad="41"/>
</signal>
<signal name="UP4RX">
<contactref element="J11" pad="P$2"/>
<contactref element="U1" pad="29"/>
</signal>
<signal name="UP4TX">
<contactref element="J11" pad="P$5"/>
<contactref element="U1" pad="30"/>
</signal>
<signal name="UP2RX">
<contactref element="J9" pad="P$2"/>
<contactref element="U1" pad="17"/>
</signal>
<signal name="UP2TX">
<contactref element="J9" pad="P$5"/>
<contactref element="U1" pad="18"/>
</signal>
<signal name="UP0RX">
<contactref element="J7" pad="P$2"/>
<contactref element="U1" pad="14"/>
</signal>
<signal name="UP0TX">
<contactref element="J7" pad="P$5"/>
<contactref element="U1" pad="13"/>
</signal>
<signal name="UP3RX">
<contactref element="J10" pad="P$2"/>
<contactref element="U1" pad="35"/>
</signal>
<signal name="UP3TX">
<contactref element="J10" pad="P$5"/>
<contactref element="U1" pad="36"/>
</signal>
<signal name="UP0STLR">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="60"/>
</signal>
<signal name="UP2STLR">
<contactref element="R6" pad="1"/>
<contactref element="U1" pad="40"/>
</signal>
<signal name="UP2STLB">
<contactref element="R7" pad="1"/>
<contactref element="U1" pad="39"/>
</signal>
<signal name="UP0STLB">
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="49"/>
</signal>
<signal name="UP3STLR">
<contactref element="R8" pad="1"/>
<contactref element="U1" pad="38"/>
</signal>
<signal name="UP3STLB">
<contactref element="R9" pad="1"/>
<contactref element="U1" pad="37"/>
</signal>
<signal name="UP4STLR">
<contactref element="R10" pad="1"/>
<contactref element="U1" pad="32"/>
</signal>
<signal name="UP4STLB">
<contactref element="R11" pad="1"/>
<contactref element="U1" pad="31"/>
</signal>
<signal name="USBDM">
<contactref element="X1" pad="D-"/>
<contactref element="J4" pad="P$1"/>
<contactref element="U1" pad="45"/>
</signal>
<signal name="USBDP">
<contactref element="X1" pad="D+"/>
<contactref element="J3" pad="P$1"/>
<contactref element="U1" pad="46"/>
</signal>
<signal name="N$6">
<contactref element="D2" pad="2"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="D1" pad="2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="D4" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="D3" pad="2"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="D6" pad="2"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="D5" pad="2"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="D8" pad="2"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="D7" pad="2"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="D10" pad="2"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="D9" pad="2"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="D13" pad="2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="D14" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$22">
<contactref element="D12" pad="2"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="D11" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="VDDCORE">
<contactref element="U1" pad="53"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="UP5RX">
<contactref element="U1" pad="43"/>
<contactref element="J1" pad="P$2"/>
</signal>
<signal name="UP5TX">
<contactref element="U1" pad="44"/>
<contactref element="J1" pad="P$5"/>
</signal>
<signal name="N$3">
<contactref element="D16" pad="2"/>
<contactref element="R17" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="D15" pad="2"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="UP5STLR">
<contactref element="R16" pad="1"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="UP5STLB">
<contactref element="R17" pad="1"/>
<contactref element="U1" pad="26"/>
</signal>
<signal name="VUSB">
<contactref element="X1" pad="VBUS"/>
<contactref element="J6" pad="P$1"/>
<contactref element="C17" pad="2"/>
<contactref element="U2" pad="3"/>
<contactref element="U2" pad="11"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="S3" pad="P$2"/>
<contactref element="S3" pad="P$5"/>
<contactref element="U2" pad="9"/>
</signal>
<signal name="BST">
<contactref element="U2" pad="10"/>
<contactref element="C19" pad="1"/>
</signal>
<signal name="VSW">
<contactref element="U2" pad="16"/>
<contactref element="U2" pad="1"/>
<contactref element="U2" pad="12"/>
<contactref element="U2" pad="13"/>
<contactref element="C19" pad="2"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="D17" pad="2"/>
<contactref element="R18" pad="2"/>
</signal>
<signal name="STLERR">
<contactref element="U1" pad="63"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="STLPACKET">
<contactref element="U1" pad="64"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="STLUSB">
<contactref element="U1" pad="3"/>
<contactref element="R18" pad="1"/>
</signal>
<signal name="STLTICKER">
<contactref element="U1" pad="4"/>
<contactref element="R13" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
