(kicad_pcb (version 20171130) (host pcbnew 5.0.1-33cea8e~68~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 88)
    (zones 0)
    (modules 10)
    (nets 19)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 Earth)
  (net 3 "Net-(IC1-Pad2)")
  (net 4 "Net-(IC1-Pad3)")
  (net 5 /RESET)
  (net 6 /MOSI)
  (net 7 /MISO)
  (net 8 /SCK)
  (net 9 /LED2)
  (net 10 /LED1)
  (net 11 "Net-(IC1-Pad12)")
  (net 12 "Net-(IC1-Pad13)")
  (net 13 "Net-(M4-Pad2)")
  (net 14 "Net-(M4-Pad6)")
  (net 15 "Net-(IC1-Pad10)")
  (net 16 "Net-(IC1-Pad11)")
  (net 17 "Net-(M1-Pad2)")
  (net 18 "Net-(M2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /SCK)
    (add_net Earth)
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M2-Pad2)")
    (add_net "Net-(M4-Pad2)")
    (add_net "Net-(M4-Pad6)")
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 184.785 118.745 90)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R2 (at 3.51028 -6.35 90) (layer F.SilkS))
    (fp_text value R_US (at 8.59028 0.635 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(M1-Pad2)"))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 5BFCE441)
    (at 194.31 118.11 270)
    (attr smd)
    (fp_text reference J1 (at 0 -2.54) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 6.985 0.635) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 /MISO))
    (pad 2 smd rect (at 2.91846 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.54 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCK))
    (pad 4 smd rect (at 2.91846 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI))
    (pad 5 smd rect (at -2.54 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 /RESET))
    (pad 6 smd rect (at 2.91846 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
  )
  (module Capacitor_SMD:C_1206_3216Metric (layer F.Cu) (tedit 5B301BBE)
    (at 196.085 102.87)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags capacitor)
    (attr smd)
    (fp_text reference C1 (at 0.765 -5.08) (layer F.SilkS))
    (fp_text value 1uF (at 0.765 -3.175) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 1 +5V))
    (pad 2 smd roundrect (at 1.4 0) (size 1.25 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.2)
      (net 2 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-SOIC14 (layer F.Cu) (tedit 200000)
    (at 193.04 109.22 270)
    (descr "SMALL OUTLINE PACKAGE")
    (tags "SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference IC1 (at -5.1435 -1.143) (layer F.SilkS))
    (fp_text value ATTINY44-SSU (at 1.27 -14.605 270) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at 0 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 5 /RESET))
    (pad 5 smd rect (at 1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 /LED1))
    (pad 6 smd rect (at 2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 /LED2))
    (pad 7 smd rect (at 3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI))
    (pad 8 smd rect (at 3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 /MISO))
    (pad 9 smd rect (at 2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCK))
    (pad 10 smd rect (at 1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 0 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at -2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at -3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 184.785 113.81486 270)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference M1 (at -11.825686 -0.411869 270) (layer F.SilkS))
    (fp_text value LED (at -1.030686 -2.316869 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 10 /LED1))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(M1-Pad2)"))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 187.325 113.665 270)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference M2 (at -11.825686 -0.411869 270) (layer F.SilkS))
    (fp_text value LED (at -7.380686 -3.586869 270) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(M2-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 /LED2))
  )
  (module fab:fab-EFOBM (layer F.Cu) (tedit 200000)
    (at 185.42 108.02874 270)
    (attr smd)
    (fp_text reference M3 (at 0 6.985 270) (layer F.SilkS))
    (fp_text value RESONATOR (at 3.175 14.605 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.34874 0) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad2)"))
    (pad 2 smd rect (at 0 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 3 smd rect (at 1.34874 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad3)"))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 200000)
    (at 200.66 109.22)
    (attr smd)
    (fp_text reference M4 (at 9.525 -0.635 90) (layer F.SilkS))
    (fp_text value FTDI-SMD-HEADER (at 4.445 0.635 270) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(M4-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(IC1-Pad13)"))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad12)"))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(M4-Pad6)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 187.325 118.745 90)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R1 (at 1.60528 -5.715 90) (layer F.SilkS))
    (fp_text value R_US (at 8.59028 0.635 90) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(M2-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 5BFCE36A)
    (at 190.5 102.87)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R3 (at 0.635 -5.715) (layer F.SilkS))
    (fp_text value 10k (at 0.635 -3.81) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 5 /RESET))
  )
)
