(kicad_pcb (version 20171130) (host pcbnew 5.0.1)
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 80)
    (zones 0)
    (modules 9)
    (nets 10)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 Earth)
  (net 3 /RESET)
  (net 4 /MOSI)
  (net 5 /MISO)
  (net 6 /SCK)
  (net 7 "Net-(M1-Pad2)")
  (net 8 "Net-(M2-Pad2)")
  (net 9 /LED)
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /LED)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /SCK)
    (add_net Earth)
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M2-Pad2)")
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 200000)
    (at 259.08 139.06754 90)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference C1 (at 1.905 -1.905 90) (layer F.SilkS))
    (fp_text value 1uF (at 5.20954 0 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.39954 0 90) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.39954 0 90) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 242.824 139.7 180)
    (attr smd)
    (fp_text reference J1 (at -0.635 -4.445 180) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 7.366 2.286 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 /MISO))
    (pad 2 smd rect (at 2.91846 -2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.54 0 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCK))
    (pad 4 smd rect (at 2.91846 0 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 5 smd rect (at -2.54 2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 /RESET))
    (pad 6 smd rect (at 2.91846 2.54 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 246.78386 132.842 180)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference M1 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value LED (at -0.35814 2.286 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 /LED))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(M1-Pad2)"))
  )
  (module fab:fab-SOIC8 (layer F.Cu) (tedit 200000)
    (at 251.32538 139.29614 180)
    (descr "WIDE PLASTIC GULL WING SMALL OUTLINE PACKAGE")
    (tags "WIDE PLASTIC GULL WING SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference M2 (at -3.4925 -1.016 270) (layer F.SilkS))
    (fp_text value ATTINY45SI (at -0.64262 22.45614 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.905 3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 3 /RESET))
    (pad 2 smd rect (at -0.64262 3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(M2-Pad2)"))
    (pad 3 smd rect (at 0.62484 3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 9 /LED))
    (pad 4 smd rect (at 1.89484 3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 5 smd rect (at 1.905 -3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 6 smd rect (at 0.635 -3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 5 /MISO))
    (pad 7 smd rect (at -0.635 -3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCK))
    (pad 8 smd rect (at -1.905 -3.15214 180) (size 0.49784 2.19964) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 254.508 146.558)
    (attr smd)
    (fp_text reference M3 (at -0.508 0) (layer F.SilkS))
    (fp_text value PINHD-2X2-SMD (at -0.254 5.08) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCK))
    (pad 2 smd rect (at 2.91846 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 3 smd rect (at -2.54 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 4 smd rect (at 2.91846 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 242.316 145.034)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R1 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value 10k (at -7.366 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCK))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 241.44986 132.842)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R2 (at -0.14986 -4.318) (layer F.SilkS))
    (fp_text value 1k (at -0.14986 -2.794) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(M1-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 256.54 139.08786 90)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R3 (at 9.29386 0 90) (layer F.SilkS))
    (fp_text value 10k (at 5.48386 -0.254 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 /RESET))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 242.16614 147.828)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R4 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value 10k (at -7.21614 0) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
)
