(kicad_pcb (version 20171130) (host pcbnew 5.0.1-33cea8e~68~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 30)
    (zones 0)
    (modules 6)
    (nets 11)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 Earth)
  (net 3 "Net-(M2-Pad4)")
  (net 4 "Net-(M2-Pad2)")
  (net 5 "Net-(M1-Pad2)")
  (net 6 "Net-(M1-Pad4)")
  (net 7 /REGULATED)
  (net 8 "Net-(IC1-Pad2)")
  (net 9 "Net-(D1-Pad2)")
  (net 10 "Net-(S1-Pad3)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.4)
    (add_net +5V)
    (add_net /REGULATED)
    (add_net Earth)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad4)")
    (add_net "Net-(M2-Pad2)")
    (add_net "Net-(M2-Pad4)")
    (add_net "Net-(S1-Pad3)")
  )
  (module fab:fab-SOT-23 (layer F.Cu) (tedit 200000)
    (at 235.458 153.5938 270)
    (descr "SMALL OUTLINE TRANSISTOR")
    (tags "SMALL OUTLINE TRANSISTOR")
    (attr smd)
    (fp_text reference IC1 (at -0.6858 -5.842 270) (layer F.SilkS))
    (fp_text value REGULATORSOT23 (at -3.2258 -3.81 270) (layer F.SilkS))
    (pad 1 smd rect (at 0.0254 1.016 270) (size 0.7874 0.889) (layers F.Cu F.Paste F.Mask)
      (net 7 /REGULATED))
    (pad 2 smd rect (at -0.9398 -1.016 270) (size 0.7874 0.889) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at 0.9906 -1.016 270) (size 0.7874 0.889) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 210.82 153.67)
    (attr smd)
    (fp_text reference M1 (at -0.635 -3.175) (layer F.SilkS))
    (fp_text value PINHD-2X2-SMD (at -3.556 5.842) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2.91846 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(M1-Pad2)"))
    (pad 3 smd rect (at -2.54 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 4 smd rect (at 2.91846 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(M1-Pad4)"))
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 228.346 153.67)
    (attr smd)
    (fp_text reference M2 (at -0.635 -3.175) (layer F.SilkS))
    (fp_text value PINHD-2X2-SMD (at 2.286 6.35) (layer F.SilkS))
    (pad 4 smd rect (at 2.91846 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(M2-Pad4)"))
    (pad 3 smd rect (at -2.54 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 2 smd rect (at 2.91846 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(M2-Pad2)"))
    (pad 1 smd rect (at -2.54 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 /REGULATED))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 219.456 154.94 180)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference D1 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value LED (at 0.508 -4.572 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 Earth))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 219.456 152.146 180)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R1 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value R_US (at 0 4.826 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 7 /REGULATED))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D1-Pad2)"))
  )
  (module fab:fab-AYZ0102AGRLC (layer F.Cu) (tedit 200000)
    (at 200.914 152.654 90)
    (attr smd)
    (fp_text reference S1 (at 0.381 -3.429 90) (layer F.SilkS))
    (fp_text value SLIDE-SWITCH (at 0.508 3.937 90) (layer F.SilkS))
    (pad 1 smd rect (at 2.49936 2.2987 90) (size 0.99822 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad2)"))
    (pad 2 smd rect (at 0 2.2987 90) (size 0.99822 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.49936 2.2987 90) (size 0.99822 1.19888) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(S1-Pad3)"))
  )
)
