(kicad_pcb (version 20171130) (host pcbnew 5.0.0)
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 141)
    (zones 0)
    (modules 25)
    (nets 64)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.45)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(IC1-Pad2)")
  (net 3 "Net-(IC1-Pad3)")
  (net 4 "Net-(IC1-Pad4)")
  (net 5 /LED1)
  (net 6 /MOSI)
  (net 7 /MISO)
  (net 8 /SCK)
  (net 9 "Net-(IC1-Pad10)")
  (net 10 "Net-(IC1-Pad12)")
  (net 11 "Net-(IC1-Pad13)")
  (net 12 "Net-(LED1-Pad1)")
  (net 13 "Net-(M1-Pad2)")
  (net 14 "Net-(M1-Pad6)")
  (net 15 "Net-(S1-Pad1)")
  (net 16 "Net-(S1-Pad3)")
  (net 17 "Net-(R3-Pad2)")
  (net 18 /LED2)
  (net 19 "Net-(LED2-Pad1)")
  (net 20 "Net-(R5-Pad2)")
  (net 21 "Net-(S2-Pad1)")
  (net 22 "Net-(S2-Pad3)")
  (net 23 "Net-(LS1-Pad1)")
  (net 24 "Net-(T1-Pad3)")
  (net 25 Earth)
  (net 26 "Net-(IC1-Pad6)")
  (net 27 /CLOCKME)
  (net 28 "Net-(IC1-Pad11)")
  (net 29 "Net-(IC2-Pad3)")
  (net 30 "Net-(IC2-Pad4)")
  (net 31 "Net-(IC2-Pad5)")
  (net 32 "Net-(IC2-Pad6)")
  (net 33 /MOSI1)
  (net 34 /MISO1)
  (net 35 /SCK1)
  (net 36 "Net-(IC2-Pad10)")
  (net 37 "Net-(IC2-Pad11)")
  (net 38 "Net-(IC2-Pad12)")
  (net 39 "Net-(IC2-Pad13)")
  (net 40 "Net-(IC3-Pad13)")
  (net 41 "Net-(IC3-Pad12)")
  (net 42 "Net-(IC3-Pad11)")
  (net 43 "Net-(IC3-Pad10)")
  (net 44 /SCK2)
  (net 45 /MISO2)
  (net 46 /MOSI2)
  (net 47 "Net-(IC3-Pad6)")
  (net 48 "Net-(IC3-Pad5)")
  (net 49 "Net-(IC3-Pad4)")
  (net 50 "Net-(IC3-Pad3)")
  (net 51 "Net-(IC4-Pad3)")
  (net 52 "Net-(IC4-Pad4)")
  (net 53 "Net-(IC4-Pad5)")
  (net 54 "Net-(IC4-Pad6)")
  (net 55 /MOSI3)
  (net 56 /MISO3)
  (net 57 /SCK3)
  (net 58 "Net-(IC4-Pad10)")
  (net 59 "Net-(IC4-Pad11)")
  (net 60 "Net-(IC4-Pad12)")
  (net 61 "Net-(IC4-Pad13)")
  (net 62 "Net-(R3-Pad1)")
  (net 63 "Net-(R5-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.45)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.4)
    (add_net +5V)
    (add_net /CLOCKME)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /MISO)
    (add_net /MISO1)
    (add_net /MISO2)
    (add_net /MISO3)
    (add_net /MOSI)
    (add_net /MOSI1)
    (add_net /MOSI2)
    (add_net /MOSI3)
    (add_net /SCK)
    (add_net /SCK1)
    (add_net /SCK2)
    (add_net /SCK3)
    (add_net Earth)
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad3)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(IC1-Pad6)")
    (add_net "Net-(IC2-Pad10)")
    (add_net "Net-(IC2-Pad11)")
    (add_net "Net-(IC2-Pad12)")
    (add_net "Net-(IC2-Pad13)")
    (add_net "Net-(IC2-Pad3)")
    (add_net "Net-(IC2-Pad4)")
    (add_net "Net-(IC2-Pad5)")
    (add_net "Net-(IC2-Pad6)")
    (add_net "Net-(IC3-Pad10)")
    (add_net "Net-(IC3-Pad11)")
    (add_net "Net-(IC3-Pad12)")
    (add_net "Net-(IC3-Pad13)")
    (add_net "Net-(IC3-Pad3)")
    (add_net "Net-(IC3-Pad4)")
    (add_net "Net-(IC3-Pad5)")
    (add_net "Net-(IC3-Pad6)")
    (add_net "Net-(IC4-Pad10)")
    (add_net "Net-(IC4-Pad11)")
    (add_net "Net-(IC4-Pad12)")
    (add_net "Net-(IC4-Pad13)")
    (add_net "Net-(IC4-Pad3)")
    (add_net "Net-(IC4-Pad4)")
    (add_net "Net-(IC4-Pad5)")
    (add_net "Net-(IC4-Pad6)")
    (add_net "Net-(LED1-Pad1)")
    (add_net "Net-(LED2-Pad1)")
    (add_net "Net-(LS1-Pad1)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad6)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(S1-Pad1)")
    (add_net "Net-(S1-Pad3)")
    (add_net "Net-(S2-Pad1)")
    (add_net "Net-(S2-Pad3)")
    (add_net "Net-(T1-Pad3)")
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 50.8 53.34 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.82 180) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 "Net-(IC1-Pad4)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 200000)
    (at 134.112 99.06)
    (attr smd)
    (fp_text reference M1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value FTDI-SMD-HEADER (at 0 0) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(M1-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad13)"))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad12)"))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(M1-Pad6)"))
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 59FED5CC)
    (at 123.952 107.173 270)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 -4.87 270) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 7 /MISO))
    (pad 2 smd rect (at 2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCK))
    (pad 4 smd rect (at 2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI))
    (pad 5 smd rect (at -2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad4)"))
    (pad 6 smd rect (at 2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 5BB7D3BE)
    (at 43.18 72.39 270)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference LED1 (at 1.905 -1.905 270) (layer F.SilkS))
    (fp_text value LED (at 2.54 1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(LED1-Pad1)"))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 56.9325 53.34)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +5V))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 25 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-EFOBM (layer F.Cu) (tedit 200000)
    (at 44.196 58.928 270)
    (attr smd)
    (fp_text reference Y1 (at 0 0 270) (layer F.SilkS))
    (fp_text value Resonator (at 0 0 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.34874 0) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 2 smd rect (at 0 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (pad 3 smd rect (at 1.34874 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad3)"))
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 68.326 40.386 180)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S2 (at 0.127 -4.318 180) (layer F.SilkS))
    (fp_text value 6MM_SWITCH6MM_SWITCH (at 0.762 4.445 180) (layer F.SilkS))
    (fp_text user 1 (at -3.048 -2.286 180) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159 180) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159 180) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159 180) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(S2-Pad1)"))
    (pad 2 smd rect (at 3.302 -2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (pad 3 smd rect (at -3.302 2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(S2-Pad3)"))
    (pad 4 smd rect (at 3.302 2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R5-Pad2)"))
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 96.52 45.466)
    (attr smd)
    (fp_text reference LS1 (at -0.635 -3.175) (layer F.SilkS))
    (fp_text value Speaker (at 0 3.175) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LS1-Pad1)"))
    (pad 2 smd rect (at 2.91846 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.54 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.91846 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask))
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 43.18 65.8225 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 "Net-(LED1-Pad1)"))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 5 /LED1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 46.99 66.04 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 270) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 /LED2))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 19 "Net-(LED2-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 82.3325 41.656)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 62 "Net-(R3-Pad1)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 17 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 46.99 72.39 270)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference LED2 (at 1.905 -1.905 270) (layer F.SilkS))
    (fp_text value LED (at 2.54 1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(LED2-Pad1)"))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
  )
  (module fab:fab-SOT-23 (layer F.Cu) (tedit 200000)
    (at 99.3394 59.436)
    (descr "SMALL OUTLINE TRANSISTOR")
    (tags "SMALL OUTLINE TRANSISTOR")
    (attr smd)
    (fp_text reference T1 (at 1.778 -3.937) (layer F.SilkS))
    (fp_text value NMOSFETSOT23 (at 2.413 -2.413) (layer F.SilkS))
    (pad 1 smd rect (at 0.0254 1.016) (size 0.7874 0.889) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(LS1-Pad1)"))
    (pad 2 smd rect (at -0.9398 -1.016) (size 0.7874 0.889) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at 0.9906 -1.016) (size 0.7874 0.889) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(T1-Pad3)"))
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 123.952 96.012)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at 0 -5.375) (layer F.SilkS))
    (fp_text value t44 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(IC1-Pad3)"))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(IC1-Pad4)"))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /CLOCKME))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad6)"))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 /MISO))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 /SCK))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 86.36 49.276 180)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S1 (at 0.127 -4.318 180) (layer F.SilkS))
    (fp_text value 6MM_SWITCH6MM_SWITCH (at 0.762 4.445 180) (layer F.SilkS))
    (fp_text user 1 (at -3.683 -2.286 180) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159 180) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159 180) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159 180) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(S1-Pad1)"))
    (pad 2 smd rect (at 3.302 -2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (pad 3 smd rect (at -3.302 2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(S1-Pad3)"))
    (pad 4 smd rect (at 3.302 2.286 180) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(R3-Pad2)"))
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 67.0925 34.036)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 20 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 63 "Net-(R5-Pad1)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 91.44 95.504)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC2 (at 0 -5.375) (layer F.SilkS))
    (fp_text value t44 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /CLOCKME))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 29 "Net-(IC2-Pad3)"))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(IC2-Pad4)"))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(IC2-Pad5)"))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC2-Pad6)"))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 33 /MOSI1))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 34 /MISO1))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 35 /SCK1))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 36 "Net-(IC2-Pad10)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 37 "Net-(IC2-Pad11)"))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 38 "Net-(IC2-Pad12)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 39 "Net-(IC2-Pad13)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 102.268 94.996)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC3 (at 0 -5.375) (layer F.SilkS))
    (fp_text value t44 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 40 "Net-(IC3-Pad13)"))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 41 "Net-(IC3-Pad12)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 42 "Net-(IC3-Pad11)"))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 43 "Net-(IC3-Pad10)"))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 44 /SCK2))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 45 /MISO2))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 46 /MOSI2))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 47 "Net-(IC3-Pad6)"))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 48 "Net-(IC3-Pad5)"))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(IC3-Pad4)"))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 50 "Net-(IC3-Pad3)"))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /CLOCKME))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 111.76 95.504)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC4 (at 0 -5.375) (layer F.SilkS))
    (fp_text value t44 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 27 /CLOCKME))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 51 "Net-(IC4-Pad3)"))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(IC4-Pad4)"))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 53 "Net-(IC4-Pad5)"))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 54 "Net-(IC4-Pad6)"))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 55 /MOSI3))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 56 /MISO3))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 57 /SCK3))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 58 "Net-(IC4-Pad10)"))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 59 "Net-(IC4-Pad11)"))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 60 "Net-(IC4-Pad12)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 61 "Net-(IC4-Pad13)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 59FED5CC)
    (at 101.6 106.68 270)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J2 (at 0 -4.87 270) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 6 smd rect (at 2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (pad 5 smd rect (at -2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 49 "Net-(IC3-Pad4)"))
    (pad 4 smd rect (at 2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 46 /MOSI2))
    (pad 3 smd rect (at -2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 44 /SCK2))
    (pad 2 smd rect (at 2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 45 /MISO2))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 59FED5CC)
    (at 90.932 106.68 270)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J3 (at 0 -4.87 270) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 34 /MISO1))
    (pad 2 smd rect (at 2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 35 /SCK1))
    (pad 4 smd rect (at 2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 33 /MOSI1))
    (pad 5 smd rect (at -2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(IC2-Pad4)"))
    (pad 6 smd rect (at 2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 59FED5CC)
    (at 112.268 106.68 270)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J4 (at 0 -4.87 270) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 0 4.87 270) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 56 /MISO3))
    (pad 2 smd rect (at 2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 57 /SCK3))
    (pad 4 smd rect (at 2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 55 /MOSI3))
    (pad 5 smd rect (at -2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 52 "Net-(IC4-Pad4)"))
    (pad 6 smd rect (at 2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 25 Earth))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 114.808 76.2)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R6 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 49 "Net-(IC3-Pad4)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 126.253001 77.809001)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R7 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +5V))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 30 "Net-(IC2-Pad4)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 126.253001 80.099001)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R8 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 52 "Net-(IC4-Pad4)"))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
)
