(kicad_pcb (version 20171130) (host pcbnew 5.0.1)
  (general
    (thickness 1.6)
    (drawings 7)
    (tracks 123)
    (zones 0)
    (modules 16)
    (nets 26)
  )
  (page A4)
  (title_block
    (title "DXH Synth 01")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.45)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 "Net-(IC1-Pad4)")
  (net 3 /LED1)
  (net 4 /MOSI)
  (net 5 /MISO)
  (net 6 /SCK)
  (net 7 "Net-(IC1-Pad12)")
  (net 8 "Net-(IC1-Pad13)")
  (net 9 "Net-(M1-Pad2)")
  (net 10 "Net-(M1-Pad6)")
  (net 11 "Net-(S1-Pad1)")
  (net 12 "Net-(S1-Pad3)")
  (net 13 "Net-(R3-Pad2)")
  (net 14 /LED2)
  (net 15 "Net-(R5-Pad2)")
  (net 16 "Net-(S2-Pad1)")
  (net 17 "Net-(S2-Pad3)")
  (net 18 Earth)
  (net 19 /XTAL1)
  (net 20 /XTAL2)
  (net 21 "Net-(LS1-Pad2)")
  (net 22 /SPEAKER)
  (net 23 /SWITCH1)
  (net 24 "Net-(LED1-Pad2)")
  (net 25 "Net-(LED2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.45)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.4)
    (add_net +5V)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net /SPEAKER)
    (add_net /SWITCH1)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net Earth)
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad4)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED2-Pad2)")
    (add_net "Net-(LS1-Pad2)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad6)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(S1-Pad1)")
    (add_net "Net-(S1-Pad3)")
    (add_net "Net-(S2-Pad1)")
    (add_net "Net-(S2-Pad3)")
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 59FED5CC)
    (at 200.66 151.115 270)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 -4.87 270) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 7.635 0) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /MISO))
    (pad 2 smd rect (at 2.525 -2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCK))
    (pad 4 smd rect (at 2.525 0 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 5 smd rect (at -2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad4)"))
    (pad 6 smd rect (at 2.525 2.54 270) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 18 Earth))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 187.198 152.4)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S1 (at 0.127 -4.318) (layer F.SilkS))
    (fp_text value 6MM_SWITCH6MM_SWITCH (at -20.828 0) (layer F.SilkS))
    (fp_text user 1 (at -3.683 -2.286) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(S1-Pad1)"))
    (pad 2 smd rect (at 3.302 -2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 Earth))
    (pad 3 smd rect (at -3.302 2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(S1-Pad3)"))
    (pad 4 smd rect (at 3.302 2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(R3-Pad2)"))
  )
  (module Package_SO:SOIC-14_3.9x8.7mm_P1.27mm (layer F.Cu) (tedit 5A02F2D3)
    (at 200.66 139.7)
    (descr "14-Lead Plastic Small Outline (SL) - Narrow, 3.90 mm Body [SOIC] (see Microchip Packaging Specification 00000049BS.pdf)")
    (tags "SOIC 1.27")
    (attr smd)
    (fp_text reference IC1 (at 0 -5.375) (layer F.SilkS))
    (fp_text value t44 (at 0 5.375) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd rect (at -2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at -2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 19 /XTAL1))
    (pad 3 smd rect (at -2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 20 /XTAL2))
    (pad 4 smd rect (at -2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(IC1-Pad4)"))
    (pad 5 smd rect (at -2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 22 /SPEAKER))
    (pad 6 smd rect (at -2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 23 /SWITCH1))
    (pad 7 smd rect (at -2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 4 /MOSI))
    (pad 8 smd rect (at 2.7 3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 5 /MISO))
    (pad 9 smd rect (at 2.7 2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 6 /SCK))
    (pad 10 smd rect (at 2.7 1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 3 /LED1))
    (pad 11 smd rect (at 2.7 0) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 14 /LED2))
    (pad 12 smd rect (at 2.7 -1.27) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 2.7 -2.54) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at 2.7 -3.81) (size 1.5 0.6) (layers F.Cu F.Paste F.Mask)
      (net 18 Earth))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 204.2525 130.81)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -6.35) (layer F.SilkS))
    (fp_text value "1 uF" (at 0.2175 -8.89) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +5V))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 Earth))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 5BB7D3BE)
    (at 207.01 147.46986 270)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference LED1 (at -0.14986 -12.7 270) (layer F.SilkS))
    (fp_text value LED (at 2.54 1.905 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 /LED1))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(LED1-Pad2)"))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 200000)
    (at 212.09 137.16)
    (attr smd)
    (fp_text reference M1 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value FTDI-SMD-HEADER (at 6.35 -1.27 90) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 18 Earth))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(M1-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(IC1-Pad13)"))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(IC1-Pad12)"))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(M1-Pad6)"))
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 198.12 130.81 180)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 6.35 180) (layer F.SilkS))
    (fp_text value 10k (at 0 8.89 180) (layer F.Fab))
    (fp_text user %R (at 0 0 180) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 2 "Net-(IC1-Pad4)"))
    (pad 2 smd roundrect (at 1.4875 0 180) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5BD4B37C)
    (at 207.01 153.8875 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -12.7 270) (layer F.SilkS))
    (fp_text value 100k (at 3.5925 -12.7 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 Earth))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 24 "Net-(LED1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-EFOBM (layer F.Cu) (tedit 200000)
    (at 193.04 138.43 270)
    (attr smd)
    (fp_text reference Y1 (at 0 0 270) (layer F.SilkS))
    (fp_text value Resonator (at -1.27 17.78) (layer F.SilkS))
    (pad 3 smd rect (at 1.34874 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 20 /XTAL2))
    (pad 2 smd rect (at 0 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 18 Earth))
    (pad 1 smd rect (at -1.34874 0) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 19 /XTAL1))
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 194.31 152.1825 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 7.8375 0 270) (layer F.SilkS))
    (fp_text value 100k (at 7.8375 1.27 270) (layer F.Fab))
    (fp_text user %R (at 0.2175 0 270) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 4 /MOSI))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 209.55 147.17014 270)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference LED2 (at 0.14986 -13.97 270) (layer F.SilkS))
    (fp_text value LED (at 2.54 1.905 270) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(LED2-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 /LED2))
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 209.55 153.8875 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -13.97 270) (layer F.SilkS))
    (fp_text value 100k (at 3.5925 -13.97 270) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 Earth))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 25 "Net-(LED2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 194.31 144.9975 270)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 2.3225 16.51) (layer F.SilkS))
    (fp_text value 100k (at 2.3225 20.32) (layer F.Fab))
    (fp_text user %R (at 0 0 270) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 15 "Net-(R5-Pad2)"))
    (pad 1 smd roundrect (at -1.4875 0 270) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 23 /SWITCH1))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 200000)
    (at 187.452 144.526)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S2 (at 0.127 -4.318) (layer F.SilkS))
    (fp_text value 6MM_SWITCH6MM_SWITCH (at -19.812 0.254) (layer F.SilkS))
    (fp_text user 1 (at -3.048 -2.286) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(S2-Pad1)"))
    (pad 2 smd rect (at 3.302 -2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 18 Earth))
    (pad 3 smd rect (at -3.302 2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(S2-Pad3)"))
    (pad 4 smd rect (at 3.302 2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(R5-Pad2)"))
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 188.33846 132.08 180)
    (attr smd)
    (fp_text reference LS1 (at 0.37846 8.89 180) (layer F.SilkS))
    (fp_text value Speaker (at 0 7.62 180) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 2.91846 -1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LS1-Pad2)"))
    (pad 3 smd rect (at -2.54 1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask))
    (pad 4 smd rect (at 2.91846 1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask))
  )
  (module fab:fab-SOT-23 (layer F.Cu) (tedit 200000)
    (at 186.69 139.3698 270)
    (descr "SMALL OUTLINE TRANSISTOR")
    (tags "SMALL OUTLINE TRANSISTOR")
    (attr smd)
    (fp_text reference T1 (at 1.778 -3.937 270) (layer F.SilkS))
    (fp_text value NMOSFETSOT23 (at 0.3302 20.32) (layer F.SilkS))
    (pad 1 smd rect (at 0.0254 1.016 270) (size 0.7874 0.889) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(LS1-Pad2)"))
    (pad 2 smd rect (at -0.9398 -1.016 270) (size 0.7874 0.889) (layers F.Cu F.Paste F.Mask)
      (net 18 Earth))
    (pad 3 smd rect (at 0.9906 -1.016 270) (size 0.7874 0.889) (layers F.Cu F.Paste F.Mask)
      (net 22 /SPEAKER))
  )
  (gr_text B (at 181.61 152.4 270) (layer F.Cu))
  (gr_text A (at 181.61 144.78 270) (layer F.Cu))
  (gr_text "SYNTH 01" (at 214.63 151.13 270) (layer F.Cu))
  (gr_line (start 180.34 157.48) (end 217.17 157.48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.34 127) (end 180.34 157.48) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.17 127) (end 180.34 127) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 217.17 157.48) (end 217.17 127) (layer Edge.Cuts) (width 0.15))
)
