(kicad_pcb (version 20171130) (host pcbnew 5.0.0)
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 0)
    (zones 0)
    (modules 8)
    (nets 30)
  )
  (page A4)
  (title_block
    (title "DXH Synth 01")
  )
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user hide)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.45)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory "./"))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /LED1)
  (net 3 /MOSI)
  (net 4 /MISO)
  (net 5 /SCK)
  (net 6 "Net-(IC1-Pad12)")
  (net 7 /LED2)
  (net 8 Earth)
  (net 9 /XTAL1)
  (net 10 /XTAL2)
  (net 11 /SPEAKER)
  (net 12 /SWITCH1)
  (net 13 "Net-(LED1-Pad2)")
  (net 14 "Net-(LED2-Pad2)")
  (net 15 "Net-(IC1-Pad22)")
  (net 16 "Net-(IC1-Pad20)")
  (net 17 "Net-(IC1-Pad19)")
  (net 18 /SWITCH2)
  (net 19 "Net-(IC1-Pad27)")
  (net 20 "Net-(IC1-Pad28)")
  (net 21 "Net-(IC1-Pad14)")
  (net 22 "Net-(IC1-Pad1)")
  (net 23 "Net-(IC1-Pad2)")
  (net 24 "Net-(IC1-Pad11)")
  (net 25 "Net-(IC1-Pad10)")
  (net 26 "Net-(IC1-Pad9)")
  (net 27 /RST)
  (net 28 "Net-(R1-Pad2)")
  (net 29 "Net-(R2-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.45)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.4)
    (add_net +5V)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RST)
    (add_net /SCK)
    (add_net /SPEAKER)
    (add_net /SWITCH1)
    (add_net /SWITCH2)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net Earth)
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad27)")
    (add_net "Net-(IC1-Pad28)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(LED1-Pad2)")
    (add_net "Net-(LED2-Pad2)")
    (add_net "Net-(R1-Pad2)")
    (add_net "Net-(R2-Pad2)")
  )
  (module Capacitor_SMD:C_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBE)
    (at 110.679001 91.683001)
    (descr "Capacitor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "capacitor handsolder")
    (attr smd)
    (fp_text reference C1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value "1 uF" (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 Earth))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +5V))
    (model ${KISYS3DMOD}/Capacitor_SMD.3dshapes/C_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Package_SO:TSOP-I-28_11.8x8mm_P0.55mm (layer F.Cu) (tedit 5AC6A6FB)
    (at 115.689001 86.163001)
    (descr "TSOP I, 28 pins, 18.8x8mm body, 0.55mm pitch, IPC-calculated pads (http://ww1.microchip.com/downloads/en/devicedoc/doc0807.pdf)")
    (tags "TSOP I 28 pins")
    (attr smd)
    (fp_text reference IC1 (at 0.5 -5.1) (layer F.SilkS))
    (fp_text value ATMEGA88-THIN (at 0 5.7) (layer F.Fab))
    (fp_text user %R (at 0.5 0) (layer F.Fab))
    (pad 7 smd rect (at -6.27 -0.275) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 9 /XTAL1))
    (pad 8 smd rect (at -6.27 0.275) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 10 /XTAL2))
    (pad 9 smd rect (at -6.27 0.825) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad9)"))
    (pad 6 smd rect (at -6.27 -0.825) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -6.27 -1.375) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 8 Earth))
    (pad 10 smd rect (at -6.27 1.375) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad10)"))
    (pad 4 smd rect (at -6.27 -1.925) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 11 smd rect (at -6.27 1.925) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad11)"))
    (pad 3 smd rect (at -6.27 -2.475) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 8 Earth))
    (pad 12 smd rect (at -6.27 2.475) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at -6.27 3.025) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 11 /SPEAKER))
    (pad 2 smd rect (at -6.27 -3.025) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad2)"))
    (pad 1 smd rect (at -6.27 -3.575) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad1)"))
    (pad 14 smd rect (at -6.27 3.575) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at 6.27 3.575) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 3 /MOSI))
    (pad 28 smd rect (at 6.27 -3.575) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(IC1-Pad28)"))
    (pad 27 smd rect (at 6.27 -3.025) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(IC1-Pad27)"))
    (pad 16 smd rect (at 6.27 3.025) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 4 /MISO))
    (pad 17 smd rect (at 6.27 2.475) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCK))
    (pad 26 smd rect (at 6.27 -2.475) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 18 /SWITCH2))
    (pad 18 smd rect (at 6.27 1.925) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 25 smd rect (at 6.27 -1.925) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 12 /SWITCH1))
    (pad 19 smd rect (at 6.27 1.375) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(IC1-Pad19)"))
    (pad 24 smd rect (at 6.27 -1.375) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 7 /LED2))
    (pad 23 smd rect (at 6.27 -0.825) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 2 /LED1))
    (pad 20 smd rect (at 6.27 0.825) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 6.27 0.275) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 8 Earth))
    (pad 22 smd rect (at 6.27 -0.275) (size 1.87 0.38) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(IC1-Pad22)"))
    (model ${KISYS3DMOD}/Package_SO.3dshapes/TSOP-I-28_11.8x8mm_P0.55mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connector_PinHeader_2.54mm:PinHeader_2x03_P2.54mm_Vertical_SMD (layer F.Cu) (tedit 59FED5CC)
    (at 115.809 103.124)
    (descr "surface-mounted straight pin header, 2x03, 2.54mm pitch, double rows")
    (tags "Surface mounted pin header SMD 2x03 2.54mm double row")
    (attr smd)
    (fp_text reference J1 (at 0 -4.87) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at 0 4.87) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 6 smd rect (at 2.525 2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 8 Earth))
    (pad 5 smd rect (at -2.525 2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 27 /RST))
    (pad 4 smd rect (at 2.525 0) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 3 /MOSI))
    (pad 3 smd rect (at -2.525 0) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCK))
    (pad 2 smd rect (at 2.525 -2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 1 smd rect (at -2.525 -2.54) (size 3.15 1) (layers F.Cu F.Paste F.Mask)
      (net 4 /MISO))
    (model ${KISYS3DMOD}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_2x03_P2.54mm_Vertical_SMD.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 127.9795 82.296)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R1 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 18 /SWITCH2))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 28 "Net-(R1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 127.9795 84.328)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R2 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 12 /SWITCH1))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 29 "Net-(R2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 128.5605 100.076)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R3 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 Earth))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 13 "Net-(LED1-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 136.652 101.092 90)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R4 (at 0 -1.82 90) (layer F.SilkS))
    (fp_text value 100k (at 0 1.82 90) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 8 Earth))
    (pad 1 smd roundrect (at -1.4875 0 90) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 14 "Net-(LED2-Pad2)"))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder (layer F.Cu) (tedit 5B301BBD)
    (at 137.1235 89.408)
    (descr "Resistor SMD 1206 (3216 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
    (tags "resistor handsolder")
    (attr smd)
    (fp_text reference R5 (at 0 -1.82) (layer F.SilkS))
    (fp_text value 10k (at 0 1.82) (layer F.Fab))
    (fp_text user %R (at 0 0) (layer F.Fab))
    (pad 2 smd roundrect (at 1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 1 +5V))
    (pad 1 smd roundrect (at -1.4875 0) (size 1.425 1.75) (layers F.Cu F.Paste F.Mask) (roundrect_rratio 0.175439)
      (net 27 /RST))
    (model ${KISYS3DMOD}/Resistor_SMD.3dshapes/R_1206_3216Metric.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
)
