(kicad_pcb (version 20171130) (host pcbnew 5.0.1)
  (general
    (thickness 1.6)
    (drawings 5)
    (tracks 146)
    (zones 0)
    (modules 15)
    (nets 24)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x010fc_ffffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 Earth)
  (net 2 "Net-(M1-Pad2)")
  (net 3 +5V)
  (net 4 "Net-(M1-Pad4)")
  (net 5 /SCK)
  (net 6 "Net-(M1-Pad6)")
  (net 7 /XTAL1)
  (net 8 /XTAL2)
  (net 9 /MOSI)
  (net 10 "Net-(J1-Pad5)")
  (net 11 /SENSE2)
  (net 12 /SENSE1)
  (net 13 /MISO)
  (net 14 "Net-(U1-Pad10)")
  (net 15 "Net-(U1-Pad11)")
  (net 16 "Net-(J3-Pad2)")
  (net 17 "Net-(M1-Pad5)")
  (net 18 "Net-(R4-Pad1)")
  (net 19 /IC-SPEAKER)
  (net 20 "Net-(R5-Pad2)")
  (net 21 "Net-(R6-Pad2)")
  (net 22 /LED1)
  (net 23 "Net-(D1-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net /IC-SPEAKER)
    (add_net /LED1)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /SCK)
    (add_net /SENSE1)
    (add_net /SENSE2)
    (add_net /XTAL1)
    (add_net /XTAL2)
    (add_net Earth)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(J1-Pad5)")
    (add_net "Net-(J3-Pad2)")
    (add_net "Net-(M1-Pad2)")
    (add_net "Net-(M1-Pad4)")
    (add_net "Net-(M1-Pad5)")
    (add_net "Net-(M1-Pad6)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad11)")
  )
  (module fab:fab-TO252 (layer F.Cu) (tedit 200000)
    (at 204.47 142.19936)
    (descr "SMALL OUTLINE TRANSISTOR")
    (tags "SMALL OUTLINE TRANSISTOR")
    (attr smd)
    (fp_text reference T1 (at -4.445 -0.635 90) (layer F.SilkS))
    (fp_text value NMOSFETSOT23 (at -11.43 -1.22936 90) (layer F.SilkS))
    (pad 3 smd rect (at 0 -2.49936) (size 5.3975 6.1976) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R6-Pad2)"))
    (pad 2 smd rect (at 2.27838 4.79806) (size 0.99822 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 1 smd rect (at -2.27838 4.79806) (size 0.99822 1.59766) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R4-Pad1)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 217.02014 133.35)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R1 (at -1.12014 -10.16) (layer F.SilkS))
    (fp_text value 10k (at 3.95986 -10.16) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad5)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 224.93986 133.35 180)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R2 (at -10.01014 0 180) (layer F.SilkS))
    (fp_text value "1 M" (at -6.20014 0 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 11 /SENSE2))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 12 /SENSE1))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 200000)
    (at 209.55 128.27 270)
    (attr smd)
    (fp_text reference M1 (at -6.35 0) (layer F.SilkS))
    (fp_text value FTDI-SMD-HEADER (at -10.16 -1.27) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 2 smd rect (at 0 -3.81 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 "Net-(M1-Pad2)"))
    (pad 3 smd rect (at 0 -1.27 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 4 smd rect (at 0 1.27 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(M1-Pad4)"))
    (pad 5 smd rect (at 0 3.81 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(M1-Pad5)"))
    (pad 6 smd rect (at 0 6.35 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(M1-Pad6)"))
  )
  (module fab:fab-EFOBM (layer F.Cu) (tedit 200000)
    (at 211.074 138.176 270)
    (attr smd)
    (fp_text reference M2 (at 0 0 270) (layer F.SilkS))
    (fp_text value RESONATOR (at 1.524 15.494 270) (layer F.SilkS))
    (pad 1 smd rect (at -1.34874 0) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 7 /XTAL1))
    (pad 2 smd rect (at 0 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 3 smd rect (at 1.34874 0 180) (size 3.8989 0.79756) (layers F.Cu F.Paste F.Mask)
      (net 8 /XTAL2))
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 200000)
    (at 217.04046 130.81)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference C1 (at -1.14046 -8.89) (layer F.SilkS))
    (fp_text value "1 uF" (at 3.93954 -8.89) (layer F.SilkS))
    (pad 1 smd rect (at -1.39954 0) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 1.39954 0) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 218.44 149.86 270)
    (attr smd)
    (fp_text reference J1 (at -0.635 -4.445 270) (layer F.SilkS))
    (fp_text value AVR-ISP-10 (at 7.62 0) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 13 /MISO))
    (pad 2 smd rect (at 2.91846 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 3 smd rect (at -2.54 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCK))
    (pad 4 smd rect (at 2.91846 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 /MOSI))
    (pad 5 smd rect (at -2.54 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 6 smd rect (at 2.91846 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-SOIC14 (layer F.Cu) (tedit 200000)
    (at 218.44 139.7 270)
    (descr "SMALL OUTLINE PACKAGE")
    (tags "SMALL OUTLINE PACKAGE")
    (attr smd)
    (fp_text reference U1 (at -2.54 -39.37) (layer F.SilkS))
    (fp_text value ATtiny44A-SSU (at 0 -22.86 270) (layer F.SilkS))
    (pad 1 smd rect (at -3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at -2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 7 /XTAL1))
    (pad 3 smd rect (at -1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 8 /XTAL2))
    (pad 4 smd rect (at 0 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(J1-Pad5)"))
    (pad 5 smd rect (at 1.27 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 19 /IC-SPEAKER))
    (pad 6 smd rect (at 2.54 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 22 /LED1))
    (pad 7 smd rect (at 3.81 2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 9 /MOSI))
    (pad 8 smd rect (at 3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 13 /MISO))
    (pad 9 smd rect (at 2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCK))
    (pad 10 smd rect (at 1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad10)"))
    (pad 11 smd rect (at 0 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad11)"))
    (pad 12 smd rect (at -1.27 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 12 /SENSE1))
    (pad 13 smd rect (at -2.54 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 11 /SENSE2))
    (pad 14 smd rect (at -3.81 -2.6035 270) (size 0.6096 2.20726) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 224.41154 129.54)
    (attr smd)
    (fp_text reference J2 (at 7.62 0) (layer F.SilkS))
    (fp_text value Conn_02x02_Counter_Clockwise (at 11.43 -15.24) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 2 smd rect (at 2.91846 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 /SENSE1))
    (pad 3 smd rect (at -2.54 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 /SENSE2))
    (pad 4 smd rect (at 2.91846 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 /SENSE1))
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 209.55 133.35 180)
    (attr smd)
    (fp_text reference J3 (at -0.635 -3.175 180) (layer F.SilkS))
    (fp_text value Speaker (at 25.4 2.54 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
    (pad 2 smd rect (at 2.91846 -1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad2)"))
    (pad 3 smd rect (at -2.54 1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad2)"))
    (pad 4 smd rect (at 2.91846 1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 +5V))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 210.96986 143.51)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R4 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value R_US (at 0 17.78) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 19 /IC-SPEAKER))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 203.2 133.35 90)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R5 (at 1.905 -1.905 90) (layer F.SilkS))
    (fp_text value 100 (at -1.27 -5.08 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 16 "Net-(J3-Pad2)"))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R5-Pad2)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 200.66 133.49986 270)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R6 (at 1.905 -1.905 270) (layer F.SilkS))
    (fp_text value 50 (at -2.68986 2.54 270) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(R6-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 270) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(R5-Pad2)"))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 210.82 149.86 180)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference D1 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value LED (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 Earth))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D1-Pad2)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 210.96986 147.32)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R7 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value 100k (at 2.54 1.905) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(D1-Pad2)"))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 22 /LED1))
  )
  (gr_line (start 198.12 156.21) (end 198.12 124.46) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 231.14 156.21) (end 198.12 156.21) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 231.14 124.46) (end 231.14 156.21) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 198.12 124.46) (end 231.14 124.46) (layer Edge.Cuts) (width 0.15))
  (gr_text "INPUT 2" (at 228.6 144.78 270) (layer F.Cu))
)
