(kicad_pcb (version 20171130) (host pcbnew 5.0.1)
  (general
    (thickness 1.6)
    (drawings 0)
    (tracks 169)
    (zones 0)
    (modules 17)
    (nets 36)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.4)
    (trace_clearance 0.4)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.3)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.8)
    (via_drill 0.4)
    (via_min_size 0.3)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.1176 0.26)
    (pad_drill 0)
    (pad_to_mask_clearance 0.051)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements 7FFFEFFF)
    (pcbplotparams
      (layerselection 0x00000_7fffffff)
      (usegerberextensions false)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 +5V)
  (net 2 /RESET)
  (net 3 Earth)
  (net 4 /MISO)
  (net 5 /SCK)
  (net 6 /MOSI)
  (net 7 /SCL)
  (net 8 /SDA)
  (net 9 "Net-(M2-Pad2)")
  (net 10 /TX)
  (net 11 /RX)
  (net 12 "Net-(M2-Pad6)")
  (net 13 /LED1)
  (net 14 /LED2)
  (net 15 /LED3)
  (net 16 /LED4)
  (net 17 "Net-(D1-Pad2)")
  (net 18 "Net-(D2-Pad2)")
  (net 19 "Net-(D3-Pad2)")
  (net 20 "Net-(D4-Pad2)")
  (net 21 "Net-(IC1-Pad1)")
  (net 22 "Net-(IC1-Pad2)")
  (net 23 "Net-(IC1-Pad7)")
  (net 24 "Net-(IC1-Pad8)")
  (net 25 "Net-(IC1-Pad9)")
  (net 26 "Net-(IC1-Pad10)")
  (net 27 "Net-(IC1-Pad11)")
  (net 28 "Net-(IC1-Pad12)")
  (net 29 "Net-(IC1-Pad13)")
  (net 30 "Net-(IC1-Pad14)")
  (net 31 "Net-(IC1-Pad18)")
  (net 32 "Net-(IC1-Pad20)")
  (net 33 "Net-(IC1-Pad32)")
  (net 34 "Net-(IC1-Pad19)")
  (net 35 "Net-(IC1-Pad22)")
  (net_class Default "This is the default net class."
    (clearance 0.4)
    (trace_width 0.4)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.4)
    (add_net +5V)
    (add_net /LED1)
    (add_net /LED2)
    (add_net /LED3)
    (add_net /LED4)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /RESET)
    (add_net /RX)
    (add_net /SCK)
    (add_net /SCL)
    (add_net /SDA)
    (add_net /TX)
    (add_net Earth)
    (add_net "Net-(D1-Pad2)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(D3-Pad2)")
    (add_net "Net-(D4-Pad2)")
    (add_net "Net-(IC1-Pad1)")
    (add_net "Net-(IC1-Pad10)")
    (add_net "Net-(IC1-Pad11)")
    (add_net "Net-(IC1-Pad12)")
    (add_net "Net-(IC1-Pad13)")
    (add_net "Net-(IC1-Pad14)")
    (add_net "Net-(IC1-Pad18)")
    (add_net "Net-(IC1-Pad19)")
    (add_net "Net-(IC1-Pad2)")
    (add_net "Net-(IC1-Pad20)")
    (add_net "Net-(IC1-Pad22)")
    (add_net "Net-(IC1-Pad32)")
    (add_net "Net-(IC1-Pad7)")
    (add_net "Net-(IC1-Pad8)")
    (add_net "Net-(IC1-Pad9)")
    (add_net "Net-(M2-Pad2)")
    (add_net "Net-(M2-Pad6)")
  )
  (net_class asdf ""
    (clearance 0.35)
    (trace_width 0.35)
    (via_dia 0.8)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (diff_pair_gap 0.25)
    (diff_pair_width 0.35)
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 285.068534 131.288648 180)
    (attr smd)
    (fp_text reference J4 (at -9.571466 0.224648 180) (layer F.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at -13.381466 -4.601352 90) (layer F.SilkS))
    (pad 4 smd rect (at 2.91846 1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.54 1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDA))
    (pad 2 smd rect (at 2.91846 -1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 1 smd rect (at -2.54 -1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL))
  )
  (module fab:fab-6MM_SWITCH (layer F.Cu) (tedit 5C04FA43)
    (at 250.952 145.288)
    (descr "OMRON SWITCH")
    (tags "OMRON SWITCH")
    (attr smd)
    (fp_text reference S1 (at 0.127 -4.318) (layer F.SilkS))
    (fp_text value 6MM_SWITCH6MM_SWITCH (at -0.762 7.112) (layer F.SilkS))
    (fp_text user 1 (at -3.683 -2.286) (layer B.SilkS))
    (fp_text user 2 (at 4.191 -2.159) (layer B.SilkS))
    (fp_text user 3 (at -3.937 2.159) (layer B.SilkS))
    (fp_text user 4 (at 4.191 2.159) (layer B.SilkS))
    (pad 1 smd rect (at -3.302 -2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 /RESET))
    (pad 2 smd rect (at 3.302 -2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 2 /RESET))
    (pad 3 smd rect (at -3.302 2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 4 smd rect (at 3.302 2.286) (size 2.286 1.524) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 243.84 144.92986 90)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference 10k1 (at 0.254 -2.54 90) (layer F.SilkS))
    (fp_text value R_US (at 2.68986 3.81 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 2 /RESET))
  )
  (module fab:fab-C1206 (layer F.Cu) (tedit 5C056D76)
    (at 283.464 143.256 180)
    (descr CAPACITOR)
    (tags CAPACITOR)
    (attr smd)
    (fp_text reference C1 (at -3.93954 7.62 180) (layer F.SilkS))
    (fp_text value C_Small (at -7.366 -0.254 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 1 smd rect (at -1.39954 0 180) (size 1.59766 1.79832) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
  )
  (module fab:fab-2X03SMD (layer F.Cu) (tedit 200000)
    (at 260.604 144.78 270)
    (attr smd)
    (fp_text reference J2 (at -0.635 -4.445 270) (layer F.SilkS))
    (fp_text value AVR-ISP-6 (at -12.7 19.304 270) (layer F.SilkS))
    (pad 1 smd rect (at -2.54 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 4 /MISO))
    (pad 2 smd rect (at 2.91846 -2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.54 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCK))
    (pad 4 smd rect (at 2.91846 0 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI))
    (pad 5 smd rect (at -2.54 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 2 /RESET))
    (pad 6 smd rect (at 2.91846 2.54 270) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
  )
  (module fab:fab-2X02SMD (layer F.Cu) (tedit 200000)
    (at 285.068534 138.146648 180)
    (attr smd)
    (fp_text reference J3 (at -1.951466 0.986648 180) (layer F.SilkS))
    (fp_text value Conn_02x02_Odd_Even (at 10.15211 5.492977 90) (layer F.SilkS))
    (pad 4 smd rect (at 2.91846 1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 3 smd rect (at -2.54 1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDA))
    (pad 2 smd rect (at 2.91846 -1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 1 smd rect (at -2.54 -1.27 180) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL))
  )
  (module fab:fab-1X06SMD (layer F.Cu) (tedit 5C04F407)
    (at 248.412 133.604)
    (attr smd)
    (fp_text reference M2 (at -2.54 0 90) (layer F.SilkS))
    (fp_text value FTDI-SMD-HEADER (at -12.7 -3.81 -90) (layer F.SilkS))
    (pad 1 smd rect (at 0 -6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 2 smd rect (at 0 -3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(M2-Pad2)"))
    (pad 3 smd rect (at 0 -1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 4 smd rect (at 0 1.27) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 10 /TX))
    (pad 5 smd rect (at 0 3.81) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 11 /RX))
    (pad 6 smd rect (at 0 6.35) (size 2.54 1.27) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(M2-Pad6)"))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 277.527188 138.202546 180)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference D2 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value LED (at -10.01014 0 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D2-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 277.527188 132.614546 180)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference D3 (at 0.14986 0 180) (layer F.SilkS))
    (fp_text value LED (at -10.01014 0 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D3-Pad2)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 5C056FDF)
    (at 271.603076 143.309092)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R2 (at 0.176924 2.740908) (layer F.SilkS))
    (fp_text value R_US (at -14.11986 0) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 13 /LED1))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad2)"))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 277.490796 143.309092 180)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference D1 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value LED (at 2.54 1.905 180) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 17 "Net-(D1-Pad2)"))
  )
  (module fab:fab-LED1206 (layer F.Cu) (tedit 200000)
    (at 277.631328 128.550546 180)
    (descr "LED 1206 PADS (STANDARD PATTERN)")
    (tags "LED 1206 PADS (STANDARD PATTERN)")
    (attr smd)
    (fp_text reference D4 (at 1.905 -1.905 180) (layer F.SilkS))
    (fp_text value LED (at 2.54 1.905 180) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad2)"))
    (pad 1 smd rect (at -1.41986 0 180) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 271.535328 138.202546)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R3 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value R_US (at 2.54 1.905) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 14 /LED2))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 18 "Net-(D2-Pad2)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 271.535328 132.614546)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R4 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value R_US (at 2.54 1.905) (layer F.SilkS))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 19 "Net-(D3-Pad2)"))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 15 /LED3))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 271.535328 128.550546)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R5 (at 1.905 -1.905) (layer F.SilkS))
    (fp_text value R_US (at 2.54 1.905) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 16 /LED4))
    (pad 2 smd rect (at 1.41986 0) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 20 "Net-(D4-Pad2)"))
  )
  (module fab:fab-TQFP32-08THIN (layer F.Cu) (tedit 5C058C03)
    (at 260.604 134.112)
    (attr smd)
    (fp_text reference IC1 (at -0.7366 -5.4864) (layer F.SilkS))
    (fp_text value ATMEGA88-THIN (at -0.5842 0.8636) (layer F.SilkS))
    (pad 1 smd rect (at -4.36626 -2.79908) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 21 "Net-(IC1-Pad1)"))
    (pad 2 smd rect (at -4.2926 -1.99898) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 22 "Net-(IC1-Pad2)"))
    (pad 3 smd rect (at -4.2926 -1.19888) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 4 smd rect (at -4.2926 -0.39878) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 5 smd rect (at -4.2926 0.39878) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 6 smd rect (at -4.2926 1.19888) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 1 +5V))
    (pad 7 smd rect (at -4.2926 1.99898) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 23 "Net-(IC1-Pad7)"))
    (pad 8 smd rect (at -4.36626 2.79908) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 24 "Net-(IC1-Pad8)"))
    (pad 9 smd rect (at -2.79908 4.36626) (size 0.26 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 25 "Net-(IC1-Pad9)"))
    (pad 10 smd rect (at -1.99898 4.2926) (size 0.26 1.27) (layers F.Cu F.Paste F.Mask)
      (net 26 "Net-(IC1-Pad10)"))
    (pad 11 smd rect (at -1.19888 4.2926) (size 0.26 1.27) (layers F.Cu F.Paste F.Mask)
      (net 27 "Net-(IC1-Pad11)"))
    (pad 12 smd rect (at -0.39878 4.2926) (size 0.26 1.27) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(IC1-Pad12)"))
    (pad 13 smd rect (at 0.39878 4.2926) (size 0.26 1.27) (layers *.Paste F.Cu F.Mask)
      (net 29 "Net-(IC1-Pad13)"))
    (pad 14 smd rect (at 1.19888 4.2926) (size 0.26 1.27) (layers F.Cu F.Paste F.Mask)
      (net 30 "Net-(IC1-Pad14)"))
    (pad 15 smd rect (at 1.99898 4.2926) (size 0.26 1.27) (layers F.Cu F.Paste F.Mask)
      (net 6 /MOSI))
    (pad 16 smd rect (at 2.79908 4.36626) (size 0.26 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 4 /MISO))
    (pad 17 smd rect (at 4.36626 2.79908) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 5 /SCK))
    (pad 18 smd rect (at 4.2926 1.99898) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 31 "Net-(IC1-Pad18)"))
    (pad 19 smd rect (at 4.2926 1.19888) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 34 "Net-(IC1-Pad19)"))
    (pad 20 smd rect (at 4.2926 0.39878) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 32 "Net-(IC1-Pad20)"))
    (pad 21 smd rect (at 4.2926 -0.39878) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 22 smd rect (at 4.2926 -1.19888) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 35 "Net-(IC1-Pad22)"))
    (pad 23 smd rect (at 4.2926 -1.99898) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 13 /LED1))
    (pad 24 smd rect (at 4.36626 -2.79908) (size 1.1176 0.26) (layers F.Cu F.Paste F.Mask)
      (net 14 /LED2))
    (pad 25 smd rect (at 2.79908 -4.36626) (size 0.26 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 15 /LED3))
    (pad 26 smd rect (at 1.99898 -4.2926) (size 0.26 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 16 /LED4))
    (pad 27 smd rect (at 1.19888 -4.2926) (size 0.26 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 8 /SDA))
    (pad 28 smd rect (at 0.39878 -4.2926) (size 0.26 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 7 /SCL))
    (pad 29 smd rect (at -0.39878 -4.2926) (size 0.26 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 2 /RESET))
    (pad 30 smd rect (at -1.19888 -4.2926) (size 0.26 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 11 /RX))
    (pad 31 smd rect (at -1.99898 -4.2926) (size 0.26 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 10 /TX))
    (pad 32 smd rect (at -2.79908 -4.36626) (size 0.26 1.1176) (layers F.Cu F.Paste F.Mask)
      (net 33 "Net-(IC1-Pad32)"))
  )
  (module fab:fab-R1206 (layer F.Cu) (tedit 200000)
    (at 278.892 148.73986 90)
    (descr RESISTOR)
    (tags RESISTOR)
    (attr smd)
    (fp_text reference R1 (at -4.93014 -0.762 90) (layer F.SilkS))
    (fp_text value 0 (at -4.93014 1.778 90) (layer F.SilkS))
    (pad 1 smd rect (at -1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
    (pad 2 smd rect (at 1.41986 0 90) (size 1.59766 1.80086) (layers F.Cu F.Paste F.Mask)
      (net 3 Earth))
  )
)
